: Public <<enumeration>> Class

Created: | 12/13/2022 5:08:28 PM
Modified: | 2/14/2023 5:54:39 PM
Project: |
Author: | FAA
Version: | 4.0.0
Phase: |
Status: | Implemented
Complexity: | Easy
Difficulty: |
Priority: |
Multiplicity: |
Advanced: |
UUID: | {C5B2BD3C-5397-4f73-B53B-59C1C69EFCFC}
Appears In: | Monitoring

The criticality RMLS-NRN assigns to each RMLS Data Point reflecting the urgency of that component failing.<br/>

- Attributes
- Advanced

Attribute
Public 1
Details:
Alias: |
Initial: |
Stereotype: |
Ordered: |
Range: |
Transient: | False
Derived: | False
IsID: | False
Notes: | Indicates the system is out of service (OTS) or possible service impacting alarm/alert. Definition based on Appendix K, NAS Event Management and Coordination (NEMAC) SOP.<br/>
Public 2
Details:
Alias: |
Initial: |
Stereotype: |
Ordered: |
Range: |
Transient: | False
Derived: | False
IsID: | False
Notes: | Imminent failure or service impacting Loss of Redundancy (LOR). Definition based on Appendix K, NAS Event Management and Coordination (NEMAC) SOP.<br/>
Public 3
Details:
Alias: |
Initial: |
Stereotype: |
Ordered: |
Range: |
Transient: | False
Derived: | False
IsID: | False
Notes: | Imminent failure or service impacting Loss of Redundancy (LOR). Definition based on Appendix K, NAS Event Management and Coordination (NEMAC) SOP.<br/>
Public 4
Details:
Alias: |
Initial: |
Stereotype: |
Ordered: |
Range: |
Transient: | False
Derived: | False
IsID: | False
Notes: | A RMLS Data Point approaching an out of tolerance threshold or an element failure not causing a service impacting LOR or OTS condition. Definition based on Appendix K, NAS Event Management and Coordination (NEMAC) SOP.<br/>
Public 5
Details:
Alias: |
Initial: |
Stereotype: |
Ordered: |
Range: |
Transient: | False
Derived: | False
IsID: | False
Notes: | A RMLS Data Point approaching an out of tolerance threshold or an element failure not causing a service impacting LOR or OTS condition. Definition based on Appendix K, NAS Event Management and Coordination (NEMAC) SOP.<br/>
Public 6
Details:
Alias: |
Initial: |
Stereotype: |
Ordered: |
Range: |
Transient: | False
Derived: | False
IsID: | False
Notes: | A RMLS Data Point approaching an out of tolerance threshold or an element failure not causing a service impacting LOR or OTS condition. Definition based on Appendix K, NAS Event Management and Coordination (NEMAC) SOP.<br/>
Public 7
Details:
Alias: |
Initial: |
Stereotype: |
Ordered: |
Range: |
Transient: | False
Derived: | False
IsID: | False
Notes: | A RMLS Data Point approaching an out of tolerance threshold or an element failure not causing a service impacting LOR or OTS condition. Definition based on Appendix K, NAS Event Management and Coordination (NEMAC) SOP.<br/>
Public 8
Details:
Alias: |
Initial: |
Stereotype: |
Ordered: |
Range: |
Transient: | False
Derived: | False
IsID: | False
Notes: | A RMLS Data Point approaching an out of tolerance threshold or an element failure not causing a service impacting LOR or OTS condition. Definition based on Appendix K, NAS Event Management and Coordination (NEMAC) SOP.<br/>
Public 9
Details:
Alias: |
Initial: |
Stereotype: |
Ordered: |
Range: |
Transient: | False
Derived: | False
IsID: | False
Notes: | A RMLS Data Point approaching an out of tolerance threshold or an element failure not causing a service impacting LOR or OTS condition. Definition based on Appendix K, NAS Event Management and Coordination (NEMAC) SOP.<br/>

Property | Value
isFinalSpecialization: | 0