complexType LogCoordination

diagram |
namespace | https://mmixm.aero/features/4
children | mx:coordinationFlag mx:coordinationStage mx:electronicFlag
used by |
element | LoggingEvent/logCoordination
annotation |
documentation
Complex type containing log coordination information, such as whether coordination is required, the status of coordination, and whether the coordination was performed.
source | <xs:complexType name="LogCoordination"> <xs:annotation> <xs:documentation>Complex type containing log coordination information, such as whether coordination is required, the status of coordination, and whether the coordination was performed.</xs:documentation> </xs:annotation> <xs:sequence> <xs:element name="coordinationFlag" type="xs:boolean" minOccurs="0" maxOccurs="1"> <xs:annotation> <xs:documentation>When "True", this field indicates that coordination is required for the maintenance activity.</xs:documentation> </xs:annotation> </xs:element> <xs:element name="coordinationStage" type="mb:CodeCoordinationRestStageDescriptionType" minOccurs="0" maxOccurs="1"> <xs:annotation> <xs:documentation>The current coordination stage of the asset, for either scheduled or unscheduled events, per RMLS NLN DB Design Document.</xs:documentation> </xs:annotation> </xs:element> <xs:element name="electronicFlag" type="xs:boolean" minOccurs="0" maxOccurs="1"> <xs:annotation> <xs:documentation>When "True", this field indicates that electronic coordination occurred for the maintenance activity.</xs:documentation> </xs:annotation> </xs:element> </xs:sequence> </xs:complexType>

element LogCoordination/coordinationFlag

diagram |
namespace | https://mmixm.aero/features/4
type | xs:boolean
properties |
minOcc | 0
maxOcc | 1
content | simple
annotation |
documentation
When "True", this field indicates that coordination is required for the maintenance activity.
source | <xs:element name="coordinationFlag" type="xs:boolean" minOccurs="0" maxOccurs="1"> <xs:annotation> <xs:documentation>When "True", this field indicates that coordination is required for the maintenance activity.</xs:documentation> </xs:annotation> </xs:element>

element LogCoordination/coordinationStage

diagram |
namespace | https://mmixm.aero/features/4
type | mb:CodeCoordinationRestStageDescriptionType
properties |
minOcc | 0
maxOcc | 1
content | simple
facets |
Kind | Value | Annotation
enumeration | Approved |
documentation
The restoration stage is coordinated and approved to restore the services of the asset to an operational state, see also TI 6140.33, Remote Monitoring and Logging System Operations Control Center (OCC) and Service Operation Center (SOC) Event Manager (EM) User's Guide.
enumeration | Callback Accepted |
documentation
A state where information is forwarded about the restoration stage for the asset in question, see also TI 6140.33, Remote Monitoring and Logging System Operations Control Center (OCC) and Service Operation Center (SOC) Event Manager (EM) User's Guide.
enumeration | Cancelled |
documentation
The scheduled/unscheduled coordination restoration stage is cancelled, see also TI 6140.33, Remote Monitoring and Logging System Operations Control Center (OCC) and Service Operation Center (SOC) Event Manager (EM) User's Guide.
enumeration | Deferred |
documentation
The scheduled/unscheduled coordination restoration stage is deferred to another time, see also TI 6140.33, Remote Monitoring and Logging System Operations Control Center (OCC) and Service Operation Center (SOC) Event Manager (EM) User's Guide.
enumeration | Delayed |
documentation
The scheduled/unscheduled coordination restoration stage is delayed to another time, see also TI 6140.33, Remote Monitoring and Logging System Operations Control Center (OCC) and Service Operation Center (SOC) Event Manager (EM) User's Guide.
enumeration | Disapproved |
documentation
The requested coordination restoration stage is not approved, see also TI 6140.33, Remote Monitoring and Logging System Operations Control Center (OCC) and Service Operation Center (SOC) Event Manager (EM) User's Guide.
enumeration | ERTS Request |
documentation
Ready to Return To Service, and an electronic Return to Service request has been initiated, see also the Electronic Return To Service (eRTS) Quick Reference Guide, and Order 6000.15, General Maintenance Handbook for National Airspace System (NAS) Facilities.
enumeration | Not Coordinated |
documentation
The unscheduled coordination restoration stage was not coordinated, see also TI 6140.33, Remote Monitoring and Logging System Operations Control Center (OCC) and Service Operation Center (SOC) Event Manager (EM) User's Guide.
enumeration | Pending Approval |
documentation
The requested coordination restoration stage is pending approval, see also TI 6140.33, Remote Monitoring and Logging System Operations Control Center (OCC) and Service Operation Center (SOC) Event Manager (EM) User's Guide.
enumeration | Pending Notification |
documentation
The requested coordination restoration stage is in a pending state, see also TI 6140.33, Remote Monitoring and Logging System Operations Control Center (OCC) and Service Operation Center (SOC) Event Manager (EM) User's Guide.
enumeration | Returned to Service |
documentation
The scheduled/unscheduled coordination restoration stage is complete and the asset has been returned to service, see also TI 6140.33, Remote Monitoring and Logging System Operations Control Center (OCC) and Service Operation Center (SOC) Event Manager (EM) User's Guide.
annotation |
documentation
The current coordination stage of the asset, for either scheduled or unscheduled events, per RMLS NLN DB Design Document.
source | <xs:element name="coordinationStage" type="mb:CodeCoordinationRestStageDescriptionType" minOccurs="0" maxOccurs="1"> <xs:annotation> <xs:documentation>The current coordination stage of the asset, for either scheduled or unscheduled events, per RMLS NLN DB Design Document.</xs:documentation> </xs:annotation> </xs:element>

element LogCoordination/electronicFlag

diagram |
namespace | https://mmixm.aero/features/4
type | xs:boolean
properties |
minOcc | 0
maxOcc | 1
content | simple
annotation |
documentation
When "True", this field indicates that electronic coordination occurred for the maintenance activity.
source | <xs:element name="electronicFlag" type="xs:boolean" minOccurs="0" maxOccurs="1"> <xs:annotation> <xs:documentation>When "True", this field indicates that electronic coordination occurred for the maintenance activity.</xs:documentation> </xs:annotation> </xs:element>

XML Schema documentation generated by XMLSpy Schema Editor http://www.altova.com/xmlspy