: Public <<XSDcomplexType>> Class

Created: | 9/22/2021 10:59:16 AM
Modified: | 12/27/2021 12:05:45 PM
Project: |
Author: | FAA
Version: | 4.0.0
Phase: |
Status: | Implemented
Complexity: | Easy
Difficulty: |
Priority: |
Multiplicity: |
Advanced: |
UUID: | {94100798-CABA-4508-8C9C-0D1A3CC4F6CB}
Appears In: | Monitoring

Complex type containing information specific to an RMLS Data Point.<br/>

- Attributes
- Associations From
- Tagged Values
- Advanced

Attribute
Public RmlsConditionCodeType conditionCode
Details:
Alias: |
Initial: |
Stereotype: |
Ordered: |
Range: | Range:0 to 1
Transient: | False
Derived: | False
IsID: | False
use=optional
Notes: | Status and condition information pertaining to an individual RMLS Data Point.<br/>
Public RmlsCriticalityCodeType criticality
Details:
Alias: |
Initial: |
Stereotype: |
Ordered: |
Range: | Range:0 to 1
Transient: | False
Derived: | False
IsID: | False
anonymousRole=false default= fixed= form= use=optional
Notes: | The criticality RMLS-NRN assigns to each RMLS Data Point reflecting the urgency of that component failing.<br/>
Public String50Type description
Details:
Alias: |
Initial: |
Stereotype: |
Ordered: |
Range: | Range:0 to 1
Transient: | False
Derived: | False
IsID: | False
anonymousRole=false default= fixed= form= use=optional
Notes: | The description of the RMLS Data Point.<br/>
Public RmlsHexId dpId
Details:
Alias: |
Initial: |
Stereotype: |
Ordered: |
Range: | Range:0 to 1
Transient: | False
Derived: | False
IsID: | False
anonymousRole=false default= fixed= form= use=optional
Notes: | The RMLS Data Point identifier, represented as a Hex Id.<br/>
Public String15Type rawValue
Details:
Alias: |
Initial: |
Stereotype: |
Ordered: |
Range: | Range:0 to 1
Transient: | False
Derived: | False
IsID: | False
anonymousRole=false
Notes: | Unmediated status or measured value of a monitored RMLS Data Point.<br/>
Public String10Type shortName
Details:
Alias: |
Initial: |
Stereotype: |
Ordered: |
Range: | Range:0 to 1
Transient: | False
Derived: | False
IsID: | False
anonymousRole=false default= fixed= form= use=optional
Notes: | The short name of the RMLS Data Point, limited to 10 characters.<br/>

Element | Source Role | Target Role
«XSDcomplexType» MonitoringEvent Class | Name: | Name: rmlsDpInformation Information specific to the RMLS concept of a Data Point.
Details:

Tag | Value
mixed | false
Details: Values: true | false Default: false Description: Determines whether this element may contain mixed element and character content. Refer to the W3C XML Schema recommendation
modelGroup | sequence
Details: Values: all | sequence | choice Default: sequence Description: Overrides the package-level default model group

Property | Value
isFinalSpecialization: | 0