complexType InterruptReport

diagram |
namespace | https://mmixm.aero/features/4
children | mx:acknowledgedBy mx:acknowledgedDateTime mx:acknowledgedFlag mx:airTrafficImpact mx:backupStatus mx:cause mx:continuityOfService mx:deviceProvenance mx:estimatedRepairDuration mx:eventType mx:failureInformation mx:followUpDateTime mx:impactLevel mx:independentEditFlag mx:interruptType mx:operationalContingency mx:pagedBackFlag mx:pagedOutFlag mx:pagedUpdateFlag mx:primeRecovery mx:remoteSaveFlag mx:reviewedFlag mx:unscheduledFlag
used by |
element | LoggingEvent/interruptReport
annotation |
documentation
Complex type containing information about a break in continuity, the loss or unavailability of an asset, regardless of duration or cause.
source | <xs:complexType name="InterruptReport"> <xs:annotation> <xs:documentation>Complex type containing information about a break in continuity, the loss or unavailability of an asset, regardless of duration or cause.</xs:documentation> </xs:annotation> <xs:sequence> <xs:element name="acknowledgedBy" type="mb:ContactInformation" minOccurs="0" maxOccurs="1"> <xs:annotation> <xs:documentation>The Strategic Event Coordination (SEC) specialist that acknowledged the interruption.</xs:documentation> </xs:annotation> </xs:element> <xs:element name="acknowledgedDateTime" type="xs:dateTime" minOccurs="0" maxOccurs="1"> <xs:annotation> <xs:documentation>The time and date of when the Strategic Event Coordination (SEC) specialist acknowledged the interruption report. (e.g. YYYY-MM-DDTHH:MM:SS)</xs:documentation> </xs:annotation> </xs:element> <xs:element name="acknowledgedFlag" type="xs:boolean" minOccurs="0" maxOccurs="1"> <xs:annotation> <xs:documentation>When "True", this field indicates the logged interruption was acknowledged by the Strategic Event Coordination (SEC) specialist.</xs:documentation> </xs:annotation> </xs:element> <xs:element name="airTrafficImpact" type="mb:AirTrafficImpactType" minOccurs="0" maxOccurs="1"> <xs:annotation> <xs:documentation>The impact level to air traffic as a result of the interruption report. (e.g. high, moderate, low, and none)</xs:documentation> </xs:annotation> </xs:element> <xs:element name="backupStatus" type="mx:BackupStatus" minOccurs="0" maxOccurs="1"> <xs:annotation> <xs:documentation>Information regarding backup systems which may have been employed during the logged interruption.</xs:documentation> </xs:annotation> </xs:element> <xs:element name="cause" type="mx:Cause" minOccurs="0" maxOccurs="1"> <xs:annotation> <xs:documentation>Information pertaining to the cause of an interruption.</xs:documentation> </xs:annotation> </xs:element> <xs:element name="continuityOfService" type="mb:ContinuityOfServiceType" minOccurs="0" maxOccurs="1"> <xs:annotation> <xs:documentation>When "True" or "Reserved", interruption impacts ILS Continuity of Service (COS), which have requirements and procedures defined in JO 6750.57, Instrument Landing System Continuity of Service Requirements and Procedures (ILS COS), per JO 6000.15.</xs:documentation> </xs:annotation> </xs:element> <xs:element name="deviceProvenance" type="mb:Provenance" minOccurs="0" maxOccurs="1"> <xs:annotation> <xs:documentation>Describes when the logged event took place, in cases where the logging device was offline and synced later.</xs:documentation> </xs:annotation> </xs:element> <xs:element name="estimatedRepairDuration" type="xs:duration" minOccurs="0" maxOccurs="1"> <xs:annotation> <xs:documentation>Total time estimated to perform the necessary repairs until the system is restored for operational use (ISO 8601 duration format).</xs:documentation> </xs:annotation> </xs:element> <xs:element name="eventType" type="mb:CodeDescriptionType" minOccurs="0" maxOccurs="1"> <xs:annotation> <xs:documentation>The type of interrupt event, as described in TI 6140.32B RMLS NOCC EM User's Guide. (e.g., "ILS FAC/Service Outage", "Loss of Redundancy", "ASDE Outage")</xs:documentation> </xs:annotation> </xs:element> <xs:element name="failureInformation" type="mb:CodeDescriptionType" minOccurs="0" maxOccurs="1"> <xs:annotation> <xs:documentation>The Service Fault Location (SFL), as defined in JO 6040.15 NAPRS. It is the location of the inoperable segment of a chain of assets, such as facilities and/or equipment, causing a service interruption.</xs:documentation> </xs:annotation> </xs:element> <xs:element name="followUpDateTime" type="xs:dateTime" minOccurs="0" maxOccurs="1"> <xs:annotation> <xs:documentation>The time and date of when an individual should follow up regarding the interruption report / event type. This time is used as a notification when a follow-up is needed on an event, as described in TI 6140.32 RMLS National Operations Control Center (NOCC) Event Manager (EM) User's Guide. (e.g. YYYY-MM-DDTHH:MM:SS)</xs:documentation> </xs:annotation> </xs:element> <xs:element name="impactLevel" type="mb:CodeDescriptionType" minOccurs="0" maxOccurs="1"> <xs:annotation> <xs:documentation>A code of the impact of level of the interruption report to AT (e.g. R8).</xs:documentation> </xs:annotation> </xs:element> <xs:element name="independentEditFlag" type="xs:boolean" minOccurs="0" maxOccurs="1"> <xs:annotation> <xs:documentation>When "True", this log entry is a child log which was edited independently of its parent.</xs:documentation> </xs:annotation> </xs:element> <xs:element name="interruptType" type="mb:CodeInterruptConditionDescriptionType" minOccurs="0" maxOccurs="1"> <xs:annotation> <xs:documentation>The interrupt condition, as defined in JO 6040.15, National Airspace Performance Reporting Services (NAPRS).</xs:documentation> </xs:annotation> </xs:element> <xs:element name="operationalContingency" type="mb:OperationalContingencyType" minOccurs="0" maxOccurs="1"> <xs:annotation> <xs:documentation>State of Operational Contingency Reporting, includes ATC-Alert notifications and ATC-Limited and ATC-Zero Operational Contingency Level (OCL) declarations as outlined in Order JO 1900.47 - Air Traffic Control Operational Readiness and Contingency Planning, for all outages/projects/events, planned or unplanned, that could cause a significant system impact, reduction in services, or reduction in capacity.</xs:documentation> </xs:annotation> </xs:element> <xs:element name="pagedBackFlag" type="xs:boolean" minOccurs="0" maxOccurs="1"> <xs:annotation> <xs:documentation>When "True", indicates the technician was paged back.</xs:documentation> </xs:annotation> </xs:element> <xs:element name="pagedOutFlag" type="xs:boolean" minOccurs="0" maxOccurs="1"> <xs:annotation> <xs:documentation>When "True", indicates the technician was paged out.</xs:documentation> </xs:annotation> </xs:element> <xs:element name="pagedUpdateFlag" type="xs:boolean" minOccurs="0" maxOccurs="1"> <xs:annotation> <xs:documentation>When "True", indicates the technician was updated via page.</xs:documentation> </xs:annotation> </xs:element> <xs:element name="primeRecovery" type="mb:CodeDescriptionType" minOccurs="0" maxOccurs="1"> <xs:annotation> <xs:documentation>The method used to recover a system.</xs:documentation> </xs:annotation> </xs:element> <xs:element name="remoteSaveFlag" type="xs:boolean" minOccurs="0" maxOccurs="1"> <xs:annotation> <xs:documentation>When "True", indicates that remote monitoring has prevented the need for a physical trip to the site.</xs:documentation> </xs:annotation> </xs:element> <xs:element name="reviewedFlag" type="xs:boolean" minOccurs="0" maxOccurs="1"> <xs:annotation> <xs:documentation>When "True", indicates the National Operations Control Center (NOCC) has reviewed the log.</xs:documentation> </xs:annotation> </xs:element> <xs:element name="unscheduledFlag" type="xs:boolean" minOccurs="0" maxOccurs="1"> <xs:annotation> <xs:documentation>When "True", indicates a maintenance event was unscheduled.</xs:documentation> </xs:annotation> </xs:element> </xs:sequence> </xs:complexType>

element InterruptReport/acknowledgedBy

diagram |
namespace | https://mmixm.aero/features/4
type | mb:ContactInformation
properties |
minOcc | 0
maxOcc | 1
content | complex
children | mb:email mb:postalAddress mb:telephoneContact
annotation |
documentation
The Strategic Event Coordination (SEC) specialist that acknowledged the interruption.
source | <xs:element name="acknowledgedBy" type="mb:ContactInformation" minOccurs="0" maxOccurs="1"> <xs:annotation> <xs:documentation>The Strategic Event Coordination (SEC) specialist that acknowledged the interruption.</xs:documentation> </xs:annotation> </xs:element>

element InterruptReport/acknowledgedDateTime

diagram |
namespace | https://mmixm.aero/features/4
type | xs:dateTime
properties |
minOcc | 0
maxOcc | 1
content | simple
annotation |
documentation
The time and date of when the Strategic Event Coordination (SEC) specialist acknowledged the interruption report. (e.g. YYYY-MM-DDTHH:MM:SS)
source | <xs:element name="acknowledgedDateTime" type="xs:dateTime" minOccurs="0" maxOccurs="1"> <xs:annotation> <xs:documentation>The time and date of when the Strategic Event Coordination (SEC) specialist acknowledged the interruption report. (e.g. YYYY-MM-DDTHH:MM:SS)</xs:documentation> </xs:annotation> </xs:element>

element InterruptReport/acknowledgedFlag

diagram |
namespace | https://mmixm.aero/features/4
type | xs:boolean
properties |
minOcc | 0
maxOcc | 1
content | simple
annotation |
documentation
When "True", this field indicates the logged interruption was acknowledged by the Strategic Event Coordination (SEC) specialist.
source | <xs:element name="acknowledgedFlag" type="xs:boolean" minOccurs="0" maxOccurs="1"> <xs:annotation> <xs:documentation>When "True", this field indicates the logged interruption was acknowledged by the Strategic Event Coordination (SEC) specialist.</xs:documentation> </xs:annotation> </xs:element>

element InterruptReport/airTrafficImpact

diagram |
namespace | https://mmixm.aero/features/4
type | mb:AirTrafficImpactType
properties |
minOcc | 0
maxOcc | 1
content | simple
facets |
Kind | Value | Annotation
enumeration | High |
documentation
High or significant impact to air traffic services, as defined in the appropriate facility SOP. For example, "high" may indicate a greater than 45 minute air traffic delay, or a ground stop is implemented beyond an internal implementation, or the event has national media interest.
enumeration | Moderate |
documentation
Moderate impact to air traffic services, as defined in the appropriate facility SOP. For example, "moderate" may indicate a 15 to 45 minute air traffic delay, or a Traffic Management Initiative (TMI) is implemented, or the event has local media interest.
enumeration | Low |
documentation
Low or negligible impact to air traffic services, as defined in the appropriate facility SOP. For example, "low" may indicate less than 15 minutes of air traffic delay, or a Traffic Management Initiative (TMI) is unnecessary or possible.
enumeration | None |
documentation
No impact to air traffic services, as defined in the appropriate facility SOP.
annotation |
documentation
The impact level to air traffic as a result of the interruption report. (e.g. high, moderate, low, and none)
source | <xs:element name="airTrafficImpact" type="mb:AirTrafficImpactType" minOccurs="0" maxOccurs="1"> <xs:annotation> <xs:documentation>The impact level to air traffic as a result of the interruption report. (e.g. high, moderate, low, and none)</xs:documentation> </xs:annotation> </xs:element>

element InterruptReport/backupStatus

diagram |
namespace | https://mmixm.aero/features/4
type | mx:BackupStatus
properties |
minOcc | 0
maxOcc | 1
content | complex
children | mx:backupCategory mx:backupEndDateTime mx:backupInUseAsPrimary mx:backupStartDateTime
annotation |
documentation
Information regarding backup systems which may have been employed during the logged interruption.
source | <xs:element name="backupStatus" type="mx:BackupStatus" minOccurs="0" maxOccurs="1"> <xs:annotation> <xs:documentation>Information regarding backup systems which may have been employed during the logged interruption.</xs:documentation> </xs:annotation> </xs:element>

element InterruptReport/cause

diagram |
namespace | https://mmixm.aero/features/4
type | mx:Cause
properties |
minOcc | 0
maxOcc | 1
content | complex
children | mx:group mx:rawText mx:subgroup
annotation |
documentation
Information pertaining to the cause of an interruption.
source | <xs:element name="cause" type="mx:Cause" minOccurs="0" maxOccurs="1"> <xs:annotation> <xs:documentation>Information pertaining to the cause of an interruption.</xs:documentation> </xs:annotation> </xs:element>

element InterruptReport/continuityOfService

diagram |
namespace | https://mmixm.aero/features/4
type | mb:ContinuityOfServiceType
properties |
minOcc | 0
maxOcc | 1
content | simple
facets |
Kind | Value | Annotation
enumeration | false |
documentation
False when the asset or outage does not require Instrument Landing System Continuity of Service (ILS COS) considerations as described in Order JO 6750.57, ILS COS Requirements and Procedures.
enumeration | reserved |
documentation
Reserved for future use. The asset or outage requires Instrument Landing System Continuity of Service (ILS COS) considerations as described in Order JO 6750.57, ILS COS Requirements and Procedures.
enumeration | true |
documentation
True when the asset or outage requires Instrument Landing System Continuity of Service (ILS COS) considerations as described in Order JO 6750.57, ILS COS Requirements and Procedures.
annotation |
documentation
When "True" or "Reserved", interruption impacts ILS Continuity of Service (COS), which have requirements and procedures defined in JO 6750.57, Instrument Landing System Continuity of Service Requirements and Procedures (ILS COS), per JO 6000.15.
source | <xs:element name="continuityOfService" type="mb:ContinuityOfServiceType" minOccurs="0" maxOccurs="1"> <xs:annotation> <xs:documentation>When "True" or "Reserved", interruption impacts ILS Continuity of Service (COS), which have requirements and procedures defined in JO 6750.57, Instrument Landing System Continuity of Service Requirements and Procedures (ILS COS), per JO 6000.15.</xs:documentation> </xs:annotation> </xs:element>

element InterruptReport/deviceProvenance

diagram |
namespace | https://mmixm.aero/features/4
type | mb:Provenance
properties |
minOcc | 0
maxOcc | 1
content | complex
children | mb:date mb:source
annotation |
documentation
Describes when the logged event took place, in cases where the logging device was offline and synced later.
source | <xs:element name="deviceProvenance" type="mb:Provenance" minOccurs="0" maxOccurs="1"> <xs:annotation> <xs:documentation>Describes when the logged event took place, in cases where the logging device was offline and synced later.</xs:documentation> </xs:annotation> </xs:element>

element InterruptReport/estimatedRepairDuration

diagram |
namespace | https://mmixm.aero/features/4
type | xs:duration
properties |
minOcc | 0
maxOcc | 1
content | simple
annotation |
documentation
Total time estimated to perform the necessary repairs until the system is restored for operational use (ISO 8601 duration format).
source | <xs:element name="estimatedRepairDuration" type="xs:duration" minOccurs="0" maxOccurs="1"> <xs:annotation> <xs:documentation>Total time estimated to perform the necessary repairs until the system is restored for operational use (ISO 8601 duration format).</xs:documentation> </xs:annotation> </xs:element>

element InterruptReport/eventType

diagram |
namespace | https://mmixm.aero/features/4
type | mb:CodeDescriptionType
properties |
minOcc | 0
maxOcc | 1
content | complex
children | mb:code mb:description
annotation |
documentation
The type of interrupt event, as described in TI 6140.32B RMLS NOCC EM User's Guide. (e.g., "ILS FAC/Service Outage", "Loss of Redundancy", "ASDE Outage")
source | <xs:element name="eventType" type="mb:CodeDescriptionType" minOccurs="0" maxOccurs="1"> <xs:annotation> <xs:documentation>The type of interrupt event, as described in TI 6140.32B RMLS NOCC EM User's Guide. (e.g., "ILS FAC/Service Outage", "Loss of Redundancy", "ASDE Outage")</xs:documentation> </xs:annotation> </xs:element>

element InterruptReport/failureInformation

diagram |
namespace | https://mmixm.aero/features/4
type | mb:CodeDescriptionType
properties |
minOcc | 0
maxOcc | 1
content | complex
children | mb:code mb:description
annotation |
documentation
The Service Fault Location (SFL), as defined in JO 6040.15 NAPRS. It is the location of the inoperable segment of a chain of assets, such as facilities and/or equipment, causing a service interruption.
source | <xs:element name="failureInformation" type="mb:CodeDescriptionType" minOccurs="0" maxOccurs="1"> <xs:annotation> <xs:documentation>The Service Fault Location (SFL), as defined in JO 6040.15 NAPRS. It is the location of the inoperable segment of a chain of assets, such as facilities and/or equipment, causing a service interruption.</xs:documentation> </xs:annotation> </xs:element>

element InterruptReport/followUpDateTime

diagram |
namespace | https://mmixm.aero/features/4
type | xs:dateTime
properties |
minOcc | 0
maxOcc | 1
content | simple
annotation |
documentation
The time and date of when an individual should follow up regarding the interruption report / event type. This time is used as a notification when a follow-up is needed on an event, as described in TI 6140.32 RMLS National Operations Control Center (NOCC) Event Manager (EM) User's Guide. (e.g. YYYY-MM-DDTHH:MM:SS)
source | <xs:element name="followUpDateTime" type="xs:dateTime" minOccurs="0" maxOccurs="1"> <xs:annotation> <xs:documentation>The time and date of when an individual should follow up regarding the interruption report / event type. This time is used as a notification when a follow-up is needed on an event, as described in TI 6140.32 RMLS National Operations Control Center (NOCC) Event Manager (EM) User's Guide. (e.g. YYYY-MM-DDTHH:MM:SS)</xs:documentation> </xs:annotation> </xs:element>

element InterruptReport/impactLevel

diagram |
namespace | https://mmixm.aero/features/4
type | mb:CodeDescriptionType
properties |
minOcc | 0
maxOcc | 1
content | complex
children | mb:code mb:description
annotation |
documentation
A code of the impact of level of the interruption report to AT (e.g. R8).
source | <xs:element name="impactLevel" type="mb:CodeDescriptionType" minOccurs="0" maxOccurs="1"> <xs:annotation> <xs:documentation>A code of the impact of level of the interruption report to AT (e.g. R8).</xs:documentation> </xs:annotation> </xs:element>

element InterruptReport/independentEditFlag

diagram |
namespace | https://mmixm.aero/features/4
type | xs:boolean
properties |
minOcc | 0
maxOcc | 1
content | simple
annotation |
documentation
When "True", this log entry is a child log which was edited independently of its parent.
source | <xs:element name="independentEditFlag" type="xs:boolean" minOccurs="0" maxOccurs="1"> <xs:annotation> <xs:documentation>When "True", this log entry is a child log which was edited independently of its parent.</xs:documentation> </xs:annotation> </xs:element>

element InterruptReport/interruptType

diagram |
namespace | https://mmixm.aero/features/4
type | mb:CodeInterruptConditionDescriptionType
properties |
minOcc | 0
maxOcc | 1
content | simple
facets |
Kind | Value | Annotation
enumeration | Full Interruption |
documentation
The interrupt condition is a full outage, see also TI 6140.33, Remote Monitoring and Logging System Operations Control Center (OCC) and Service Operation Center (SOC) Event Manager (EM) User's Guide.
enumeration | Informational Entry |
documentation
The log entry is for coordination purposes only, see also TI 6140.33, Remote Monitoring and Logging System Operations Control Center (OCC) and Service Operation Center (SOC) Event Manager (EM) User's Guide.
enumeration | Reduced Facility/Service Interruption |
documentation
The interruption or outage has resulted in a reduced service condition, see also TI 6140.33, Remote Monitoring and Logging System Operations Control Center (OCC) and Service Operation Center (SOC) Event Manager (EM) User's Guide.
enumeration | Reduced System/Equipment |
documentation
The interruption or outage has resulted in a reduced equipment condition, see also TI 6140.33, Remote Monitoring and Logging System Operations Control Center (OCC) and Service Operation Center (SOC) Event Manager (EM) User's Guide.
annotation |
documentation
The interrupt condition, as defined in JO 6040.15, National Airspace Performance Reporting Services (NAPRS).
source | <xs:element name="interruptType" type="mb:CodeInterruptConditionDescriptionType" minOccurs="0" maxOccurs="1"> <xs:annotation> <xs:documentation>The interrupt condition, as defined in JO 6040.15, National Airspace Performance Reporting Services (NAPRS).</xs:documentation> </xs:annotation> </xs:element>

element InterruptReport/operationalContingency

diagram |
namespace | https://mmixm.aero/features/4
type | mb:OperationalContingencyType
properties |
minOcc | 0
maxOcc | 1
content | simple
facets |
Kind | Value | Annotation
enumeration | ATC-Zero |
documentation
Per JO 1900.47 Air Traffic Control Operational Readiness and Contingency Planning, ATC-ZERO is an Operational Contingency Level (OCL) declared when any of the following occur: a. A facility is unable to provide services, or traffic flow management in the case of the ATCSCC, during published operating hours with its facility personnel or with personnel that routinely work the transferred airspace or services from either the normal location or any alternate location. b. A facility transfers services to another facility whose personnel do not routinely work the transferred airspace or services.
enumeration | ATC-Limited |
documentation
Per JO 1900.47 Air Traffic Control Operational Readiness and Contingency Planning, ATC-Limited is an Operational Contingency Level (OCL) declared when any of the following occur: a. A combined Tower/TRACON ("up/down") facility is unable to provide services from one area (Tower Cab or TRACON), but the other area remains in operation. b. A multi-area facility is unable to provide services from one or more areas, but other areas remain in operation. c. A facility is providing services with its facility personnel from an alternate location. d. A facility has transferred all services during published operating hours to another facility whose personnel routinely work the transferred airspace or services.
enumeration | ATC-Alert |
documentation
A precautionary notification made when a facility remains in normal operations but anticipates disruptive condition(s) or experiences a loss of redundancy that may indicate a potential interruption in services, per JO 1900.47 Air Traffic Control Operational Readiness and Contingency Planning.
annotation |
documentation
State of Operational Contingency Reporting, includes ATC-Alert notifications and ATC-Limited and ATC-Zero Operational Contingency Level (OCL) declarations as outlined in Order JO 1900.47 - Air Traffic Control Operational Readiness and Contingency Planning, for all outages/projects/events, planned or unplanned, that could cause a significant system impact, reduction in services, or reduction in capacity.
source | <xs:element name="operationalContingency" type="mb:OperationalContingencyType" minOccurs="0" maxOccurs="1"> <xs:annotation> <xs:documentation>State of Operational Contingency Reporting, includes ATC-Alert notifications and ATC-Limited and ATC-Zero Operational Contingency Level (OCL) declarations as outlined in Order JO 1900.47 - Air Traffic Control Operational Readiness and Contingency Planning, for all outages/projects/events, planned or unplanned, that could cause a significant system impact, reduction in services, or reduction in capacity.</xs:documentation> </xs:annotation> </xs:element>

element InterruptReport/pagedBackFlag

diagram |
namespace | https://mmixm.aero/features/4
type | xs:boolean
properties |
minOcc | 0
maxOcc | 1
content | simple
annotation |
documentation
When "True", indicates the technician was paged back.
source | <xs:element name="pagedBackFlag" type="xs:boolean" minOccurs="0" maxOccurs="1"> <xs:annotation> <xs:documentation>When "True", indicates the technician was paged back.</xs:documentation> </xs:annotation> </xs:element>

element InterruptReport/pagedOutFlag

diagram |
namespace | https://mmixm.aero/features/4
type | xs:boolean
properties |
minOcc | 0
maxOcc | 1
content | simple
annotation |
documentation
When "True", indicates the technician was paged out.
source | <xs:element name="pagedOutFlag" type="xs:boolean" minOccurs="0" maxOccurs="1"> <xs:annotation> <xs:documentation>When "True", indicates the technician was paged out.</xs:documentation> </xs:annotation> </xs:element>

element InterruptReport/pagedUpdateFlag

diagram |
namespace | https://mmixm.aero/features/4
type | xs:boolean
properties |
minOcc | 0
maxOcc | 1
content | simple
annotation |
documentation
When "True", indicates the technician was updated via page.
source | <xs:element name="pagedUpdateFlag" type="xs:boolean" minOccurs="0" maxOccurs="1"> <xs:annotation> <xs:documentation>When "True", indicates the technician was updated via page.</xs:documentation> </xs:annotation> </xs:element>

element InterruptReport/primeRecovery

diagram |
namespace | https://mmixm.aero/features/4
type | mb:CodeDescriptionType
properties |
minOcc | 0
maxOcc | 1
content | complex
children | mb:code mb:description
annotation |
documentation
The method used to recover a system.
source | <xs:element name="primeRecovery" type="mb:CodeDescriptionType" minOccurs="0" maxOccurs="1"> <xs:annotation> <xs:documentation>The method used to recover a system.</xs:documentation> </xs:annotation> </xs:element>

element InterruptReport/remoteSaveFlag

diagram |
namespace | https://mmixm.aero/features/4
type | xs:boolean
properties |
minOcc | 0
maxOcc | 1
content | simple
annotation |
documentation
When "True", indicates that remote monitoring has prevented the need for a physical trip to the site.
source | <xs:element name="remoteSaveFlag" type="xs:boolean" minOccurs="0" maxOccurs="1"> <xs:annotation> <xs:documentation>When "True", indicates that remote monitoring has prevented the need for a physical trip to the site.</xs:documentation> </xs:annotation> </xs:element>

element InterruptReport/reviewedFlag

diagram |
namespace | https://mmixm.aero/features/4
type | xs:boolean
properties |
minOcc | 0
maxOcc | 1
content | simple
annotation |
documentation
When "True", indicates the National Operations Control Center (NOCC) has reviewed the log.
source | <xs:element name="reviewedFlag" type="xs:boolean" minOccurs="0" maxOccurs="1"> <xs:annotation> <xs:documentation>When "True", indicates the National Operations Control Center (NOCC) has reviewed the log.</xs:documentation> </xs:annotation> </xs:element>

element InterruptReport/unscheduledFlag

diagram |
namespace | https://mmixm.aero/features/4
type | xs:boolean
properties |
minOcc | 0
maxOcc | 1
content | simple
annotation |
documentation
When "True", indicates a maintenance event was unscheduled.
source | <xs:element name="unscheduledFlag" type="xs:boolean" minOccurs="0" maxOccurs="1"> <xs:annotation> <xs:documentation>When "True", indicates a maintenance event was unscheduled.</xs:documentation> </xs:annotation> </xs:element>

XML Schema documentation generated by XMLSpy Schema Editor http://www.altova.com/xmlspy