: Public <<XSDcomplexType>> Class

Created: | 1/31/2024 7:27:45 PM
Modified: | 8/7/2024 4:51:26 PM
Project: |
Author: | FAA
Version: | 4.0.0
Phase: |
Status: | Implemented
Complexity: | Easy
Difficulty: |
Priority: |
Multiplicity: |
Advanced: |
UUID: | {FB8BB395-D62C-476e-A2C1-0B1626DFF1FB}
Appears In: | Logging

Complex type containing information about a break in continuity, the loss or unavailability of an asset, regardless of duration or cause.<br/>

- Attributes
- Associations To
- Associations From
- Tagged Values
- Advanced

Attribute
Public ContactInformation acknowledgedBy
Details:
Alias: |
Initial: |
Stereotype: |
Ordered: |
Range: | Range:0 to 1
Transient: | False
Derived: | False
IsID: | False
position=1
Notes: | The Strategic Event Coordination (SEC) specialist that acknowledged the interruption.<br/>
Public dateTime acknowledgedDateTime
Details:
Alias: |
Initial: |
Stereotype: |
Ordered: |
Range: | Range:0 to 1
Transient: | False
Derived: | False
IsID: | False
position=2
Notes: | The time and date of when the Strategic Event Coordination (SEC) specialist acknowledged the interruption report. (e.g. YYYY-MM-DDTHH:MM:SS)<br/>
Public boolean acknowledgedFlag
Details:
Alias: |
Initial: |
Stereotype: |
Ordered: |
Range: | Range:0 to 1
Transient: | False
Derived: | False
IsID: | False
position=3
Notes: | When "True", this field indicates the logged interruption was acknowledged by the Strategic Event Coordination (SEC) specialist.<br/>
Public AirTrafficImpactType airTrafficImpact
Details:
Alias: |
Initial: |
Stereotype: |
Ordered: |
Range: | Range:0 to 1
Transient: | False
Derived: | False
IsID: | False
position=4
Notes: | The impact level to air traffic as a result of the interruption report. (e.g. high, moderate, low, and none)<br/>
Public ContinuityOfServiceType continuityOfService
Details:
Alias: |
Initial: |
Stereotype: |
Ordered: |
Range: | Range:0 to 1
Transient: | False
Derived: | False
IsID: | False
position=7
Notes: | When "True" or "Reserved", interruption impacts ILS Continuity of Service (COS), which have requirements and procedures defined in JO 6750.57, Instrument Landing System Continuity of Service Requirements and Procedures (ILS COS), per JO 6000.15.<br/>
Public Provenance deviceProvenance
Details:
Alias: |
Initial: |
Stereotype: |
Ordered: |
Range: | Range:0 to 1
Transient: | False
Derived: | False
IsID: | False
Notes: | Describes when the logged event took place, in cases where the logging device was offline and synced later.<br/>
Public duration estimatedRepairDuration
Details:
Alias: |
Initial: |
Stereotype: |
Ordered: |
Range: | Range:0 to 1
Transient: | False
Derived: | False
IsID: | False
Notes: | Total time estimated to perform the necessary repairs until the system is restored for operational use (ISO 8601 duration format).<br/>
Public CodeDescriptionType eventType
Details:
Alias: |
Initial: |
Stereotype: |
Ordered: |
Range: | Range:0 to 1
Transient: | False
Derived: | False
IsID: | False
Notes: | The type of interrupt event, as described in TI 6140.32B RMLS NOCC EM User's Guide. (e.g., "ILS FAC/Service Outage", "Loss of Redundancy", "ASDE Outage")<br/>
Public CodeDescriptionType failureInformation
Details:
Alias: |
Initial: |
Stereotype: |
Ordered: |
Range: | Range:0 to 1
Transient: | False
Derived: | False
IsID: | False
Notes: | The Service Fault Location (SFL), as defined in JO 6040.15 NAPRS. It is the location of the inoperable segment of a chain of assets, such as facilities and/or equipment, causing a service interruption.<br/>
Public dateTime followUpDateTime
Details:
Alias: |
Initial: |
Stereotype: |
Ordered: |
Range: | Range:0 to 1
Transient: | False
Derived: | False
IsID: | False
Notes: | The time and date of when an individual should follow up regarding the interruption report / event type. This time is used as a notification when a follow-up is needed on an event, as described in TI 6140.32 RMLS National Operations Control Center (NOCC) Event Manager (EM) User's Guide. (e.g. YYYY-MM-DDTHH:MM:SS)<br/>
Public CodeDescriptionType impactLevel
Details:
Alias: |
Initial: |
Stereotype: |
Ordered: |
Range: | Range:0 to 1
Transient: | False
Derived: | False
IsID: | False
Notes: | A code of the impact of level of the interruption report to AT (e.g. R8).<br/>
Public boolean independentEditFlag
Details:
Alias: |
Initial: |
Stereotype: |
Ordered: |
Range: | Range:0 to 1
Transient: | False
Derived: | False
IsID: | False
Notes: | When "True", this log entry is a child log which was edited independently of its parent.<br/>
Public CodeInterruptConditionDescriptionType interruptType
Details:
Alias: |
Initial: |
Stereotype: |
Ordered: |
Range: | Range:0 to 1
Transient: | False
Derived: | False
IsID: | False
Notes: | The interrupt condition, as defined in JO 6040.15, National Airspace Performance Reporting Services (NAPRS).<br/>
Public OperationalContingencyType operationalContingency
Details:
Alias: |
Initial: |
Stereotype: |
Ordered: |
Range: | Range:0 to 1
Transient: | False
Derived: | False
IsID: | False
Notes: | State of Operational Contingency Reporting, includes ATC-Alert notifications and ATC-Limited and ATC-Zero Operational Contingency Level (OCL) declarations as outlined in Order JO 1900.47 - Air Traffic Control Operational Readiness and Contingency Planning, for all outages/projects/events, planned or unplanned, that could cause a significant system impact, reduction in services, or reduction in capacity.<br/>
Public boolean pagedBackFlag
Details:
Alias: |
Initial: |
Stereotype: |
Ordered: |
Range: | Range:0 to 1
Transient: | False
Derived: | False
IsID: | False
Notes: | When "True", indicates the technician was paged back.<br/>
Public boolean pagedOutFlag
Details:
Alias: |
Initial: |
Stereotype: |
Ordered: |
Range: | Range:0 to 1
Transient: | False
Derived: | False
IsID: | False
Notes: | When "True", indicates the technician was paged out.<br/>
Public boolean pagedUpdateFlag
Details:
Alias: |
Initial: |
Stereotype: |
Ordered: |
Range: | Range:0 to 1
Transient: | False
Derived: | False
IsID: | False
Notes: | When "True", indicates the technician was updated via page.<br/>
Public CodeDescriptionType primeRecovery
Details:
Alias: |
Initial: |
Stereotype: |
Ordered: |
Range: | Range:0 to 1
Transient: | False
Derived: | False
IsID: | False
Notes: | The method used to recover a system.<br/>
Public boolean remoteSaveFlag
Details:
Alias: |
Initial: |
Stereotype: |
Ordered: |
Range: | Range:0 to 1
Transient: | False
Derived: | False
IsID: | False
Notes: | When "True", indicates that remote monitoring has prevented the need for a physical trip to the site.<br/>
Public boolean reviewedFlag
Details:
Alias: |
Initial: |
Stereotype: |
Ordered: |
Range: | Range:0 to 1
Transient: | False
Derived: | False
IsID: | False
Notes: | When "True", indicates the National Operations Control Center (NOCC) has reviewed the log.<br/>
Public boolean unscheduledFlag
Details:
Alias: |
Initial: |
Stereotype: |
Ordered: |
Range: | Range:0 to 1
Transient: | False
Derived: | False
IsID: | False
Notes: | When "True", indicates a maintenance event was unscheduled.<br/>

Element | Source Role | Target Role
«XSDcomplexType» BackupStatus Class | Name: | Name: backupStatus Information regarding backup systems which may have been employed during the logged interruption.
Details:
«XSDcomplexType» Cause Class | Name: | Name: cause Information pertaining to the cause of an interruption.
Details:

Element | Source Role | Target Role
«XSDcomplexType» LoggingEvent Class | Name: | Name: interruptReport Information about a break in continuity, the loss or unavailability of an asset, regardless of duration or cause.
Details:

Tag | Value
mixed | false
Details: Values: true | false Default: false Description: Determines whether this element may contain mixed element and character content. Refer to the W3C XML Schema recommendation
modelGroup | sequence
Details: Values: all | sequence | choice Default: sequence Description: Overrides the package-level default model group
nillable | false
Details: Values: true | false Default: false Description: As defined by XML Schema specification

Property | Value
isFinalSpecialization: | 0