simpleType RmlsCriticalityCodeType

namespace | https://mmixm.aero/features/4
type | restriction of xs:string
properties |
base | xs:string
used by |
element | RmlsDpInformation/criticality
facets |
Kind | Value | Annotation
enumeration | 1 |
documentation
Indicates the system is out of service (OTS) or possible service impacting alarm/alert. Definition based on Appendix K, NAS Event Management and Coordination (NEMAC) SOP.
enumeration | 2 |
documentation
Imminent failure or service impacting Loss of Redundancy (LOR). Definition based on Appendix K, NAS Event Management and Coordination (NEMAC) SOP.
enumeration | 3 |
documentation
Imminent failure or service impacting Loss of Redundancy (LOR). Definition based on Appendix K, NAS Event Management and Coordination (NEMAC) SOP.
enumeration | 4 |
documentation
A RMLS Data Point approaching an out of tolerance threshold or an element failure not causing a service impacting LOR or OTS condition. Definition based on Appendix K, NAS Event Management and Coordination (NEMAC) SOP.
enumeration | 5 |
documentation
A RMLS Data Point approaching an out of tolerance threshold or an element failure not causing a service impacting LOR or OTS condition. Definition based on Appendix K, NAS Event Management and Coordination (NEMAC) SOP.
enumeration | 6 |
documentation
A RMLS Data Point approaching an out of tolerance threshold or an element failure not causing a service impacting LOR or OTS condition. Definition based on Appendix K, NAS Event Management and Coordination (NEMAC) SOP.
enumeration | 7 |
documentation
A RMLS Data Point approaching an out of tolerance threshold or an element failure not causing a service impacting LOR or OTS condition. Definition based on Appendix K, NAS Event Management and Coordination (NEMAC) SOP.
enumeration | 8 |
documentation
A RMLS Data Point approaching an out of tolerance threshold or an element failure not causing a service impacting LOR or OTS condition. Definition based on Appendix K, NAS Event Management and Coordination (NEMAC) SOP.
enumeration | 9 |
documentation
A RMLS Data Point approaching an out of tolerance threshold or an element failure not causing a service impacting LOR or OTS condition. Definition based on Appendix K, NAS Event Management and Coordination (NEMAC) SOP.
annotation |
documentation
The criticality RMLS-NRN assigns to each RMLS Data Point reflecting the urgency of that component failing.
source | <xs:simpleType name="RmlsCriticalityCodeType"> <xs:annotation> <xs:documentation>The criticality RMLS-NRN assigns to each RMLS Data Point reflecting the urgency of that component failing.</xs:documentation> </xs:annotation> <xs:restriction base="xs:string"> <xs:enumeration value="1"> <xs:annotation> <xs:documentation>Indicates the system is out of service (OTS) or possible service impacting alarm/alert. Definition based on Appendix K, NAS Event Management and Coordination (NEMAC) SOP.</xs:documentation> </xs:annotation> </xs:enumeration> <xs:enumeration value="2"> <xs:annotation> <xs:documentation>Imminent failure or service impacting Loss of Redundancy (LOR). Definition based on Appendix K, NAS Event Management and Coordination (NEMAC) SOP.</xs:documentation> </xs:annotation> </xs:enumeration> <xs:enumeration value="3"> <xs:annotation> <xs:documentation>Imminent failure or service impacting Loss of Redundancy (LOR). Definition based on Appendix K, NAS Event Management and Coordination (NEMAC) SOP.</xs:documentation> </xs:annotation> </xs:enumeration> <xs:enumeration value="4"> <xs:annotation> <xs:documentation>A RMLS Data Point approaching an out of tolerance threshold or an element failure not causing a service impacting LOR or OTS condition. Definition based on Appendix K, NAS Event Management and Coordination (NEMAC) SOP.</xs:documentation> </xs:annotation> </xs:enumeration> <xs:enumeration value="5"> <xs:annotation> <xs:documentation>A RMLS Data Point approaching an out of tolerance threshold or an element failure not causing a service impacting LOR or OTS condition. Definition based on Appendix K, NAS Event Management and Coordination (NEMAC) SOP.</xs:documentation> </xs:annotation> </xs:enumeration> <xs:enumeration value="6"> <xs:annotation> <xs:documentation>A RMLS Data Point approaching an out of tolerance threshold or an element failure not causing a service impacting LOR or OTS condition. Definition based on Appendix K, NAS Event Management and Coordination (NEMAC) SOP.</xs:documentation> </xs:annotation> </xs:enumeration> <xs:enumeration value="7"> <xs:annotation> <xs:documentation>A RMLS Data Point approaching an out of tolerance threshold or an element failure not causing a service impacting LOR or OTS condition. Definition based on Appendix K, NAS Event Management and Coordination (NEMAC) SOP.</xs:documentation> </xs:annotation> </xs:enumeration> <xs:enumeration value="8"> <xs:annotation> <xs:documentation>A RMLS Data Point approaching an out of tolerance threshold or an element failure not causing a service impacting LOR or OTS condition. Definition based on Appendix K, NAS Event Management and Coordination (NEMAC) SOP.</xs:documentation> </xs:annotation> </xs:enumeration> <xs:enumeration value="9"> <xs:annotation> <xs:documentation>A RMLS Data Point approaching an out of tolerance threshold or an element failure not causing a service impacting LOR or OTS condition. Definition based on Appendix K, NAS Event Management and Coordination (NEMAC) SOP.</xs:documentation> </xs:annotation> </xs:enumeration> </xs:restriction> </xs:simpleType>

XML Schema documentation generated by XMLSpy Schema Editor http://www.altova.com/xmlspy