: Public <<XSDcomplexType>> Class

Created: | 5/21/2024 4:25:58 PM
Modified: | 7/30/2024 2:40:12 PM
Project: |
Author: | FAA
Version: | 4.0.0
Phase: |
Status: | Implemented
Complexity: | Easy
Difficulty: |
Priority: |
Multiplicity: |
Advanced: |
UUID: | {C93EAA4A-E104-4944-AA08-CCFCF7997E5D}
Appears In: | Asset, Logging

Complex type containing logging event information.<br/>

- Attributes
- Associations To
- Associations From
- Tagged Values
- Advanced

Attribute
Public AdditionalInformation additionalInformation
Details:
Alias: |
Initial: |
Stereotype: |
Ordered: |
Range: | Range:0 to 1
Transient: | False
Derived: | False
IsID: | False
position=1
Notes: | Additional information about a Logging event.<br/>
Public String4000Type comment
Details:
Alias: |
Initial: |
Stereotype: |
Ordered: |
Range: | Range:0 to 1
Transient: | False
Derived: | False
IsID: | False
position=5
Notes: | Free text comment on the logging event, and can include detailed information, per JO 6040.15 National Airspace Performance Reporting Services (NAPRS).<br/>
Public ContactInformation createdBy
Details:
Alias: |
Initial: |
Stereotype: |
Ordered: |
Range: | Range:0 to 1
Transient: | False
Derived: | False
IsID: | False
position=6
Notes: | The contact information of the person who created the log entry.<br/>
Public dateTime createdDateTime
Details:
Alias: |
Initial: |
Stereotype: |
Ordered: |
Range: | Range:0 to 1
Transient: | False
Derived: | False
IsID: | False
position=7
Notes: | The time and date of when the log data was created.<br/>
Public Location creatorLocation
Details:
Alias: |
Initial: |
Stereotype: |
Ordered: |
Range: | Range:0 to 1
Transient: | False
Derived: | False
IsID: | False
position=8
Notes: | The organization/location of where the log data was created.<br/>
Public FsepOperationalInformation fsepOperationalInformationSnapshot
Details:
Alias: |
Initial: |
Stereotype: |
Ordered: |
Range: | Range:0 to 1
Transient: | False
Derived: | False
IsID: | False
position=10
Notes: | A static capture of the FSEP operational information associated with an asset, current at the time the event was logged.<br/>
Public Integer22Type logId
Details:
Alias: |
Initial: |
Stereotype: |
Ordered: |
Range: | Range:0 to 1
Transient: | False
Derived: | False
IsID: | False
position=14
Notes: | This field contains the ID number of the log entry.<br/>
Public ContactInformation modifiedBy
Details:
Alias: |
Initial: |
Stereotype: |
Ordered: |
Range: | Range:0 to 1
Transient: | False
Derived: | False
IsID: | False
position=16
Notes: | The contact information of the person that modified the log data.<br/>
Public dateTime modifiedDateTime
Details:
Alias: |
Initial: |
Stereotype: |
Ordered: |
Range: | Range:0 to 1
Transient: | False
Derived: | False
IsID: | False
position=17
Notes: | The time and date of when the log entry was modified / updated. (e.g. YYYY-MM-DDTHH:MM:SS)<br/>
Public String1Type reportLevel
Details:
Alias: |
Initial: |
Stereotype: |
Ordered: |
Range: | Range:0 to 1
Transient: | False
Derived: | False
IsID: | False
position=20
Notes: | The report level of the log entry as defined in TI 6140.31 RMLS Peabody User's Guide. "N" indicates reportable per Order 6040.15 (NAPRS), "L" indicates reportable by local policy.<br/>
Public CodeLogStatusDescriptionType status
Details:
Alias: |
Initial: |
Stereotype: |
Ordered: |
Range: | Range:0 to 1
Transient: | False
Derived: | False
IsID: | False
position=21
Notes: | The status of the log entry, per TI 6140.33 OCC/SOC Event Manager User's Guide. (e.g. Closed/ open / void)<br/>
Public String255Type summary
Details:
Alias: |
Initial: |
Stereotype: |
Ordered: |
Range: | Range:0 to 1
Transient: | False
Derived: | False
IsID: | False
position=22
Notes: | A free-text summary of the logged event or activity conducted.<br/>

Element | Source Role | Target Role
«XSDcomplexType» LogCoordination Class | Name: | Name: logCoordination Log coordination information, such as whether coordination is required, the status of coordination, and whether the coordination was performed.
Details:
«XSDcomplexType» MaintenanceActivity Class | Name: | Name: maintenanceActivity Maintenance activity information, including start and end time of the maintenance activity.
Details:
«XSDcomplexType» LoggingCode Class | Name: | Name: loggingCode Code information for a logging event, including the code category, the maintenance action code, and the supplemental code.
Details:
«XSDcomplexType» AssignmentInformation Class | Name: | Name: assignmentInformation Information about assigned group and specialist.
Details:
«XSDcomplexType» Alarm Class | Name: | Name: alarm Alarm information associated with a logging event.
Details:
«XSDcomplexType» ArrivalDeparture Class | Name: | Name: arrivalDeparture Technicians' travel information, such as arrival and departure times, and travel duration.
Details:
«XSDcomplexType» PeriodicMaintenance Class | Name: | Name: periodicMaintenance Information about a periodic maintenance logging event.
Details:
«XSDcomplexType» NotamInformation Class | Name: | Name: notamInformation Information about associated NOTAMs.
Details:
«XSDcomplexType» InterruptReport Class | Name: | Name: interruptReport Information about a break in continuity, the loss or unavailability of an asset, regardless of duration or cause.
Details:
«XSDcomplexType» EquipmentModification Class | Name: | Name: equipmentModification Information about an equipment modification event.
Details:

Element | Source Role | Target Role
«XSDcomplexType» Asset Class | Name: | Name: loggingEvent Logging event associated with a specific asset.
Details:

Tag | Value
mixed | false
Details: Values: true | false Default: false Description: Determines whether this element may contain mixed element and character content. Refer to the W3C XML Schema recommendation
modelGroup | sequence
Details: Values: all | sequence | choice Description: Overrides the package-level default model group

Property | Value
isFinalSpecialization: | 0