simpleType RmlsConditionCodeType

namespace | https://mmixm.aero/features/4
type | restriction of xs:string
properties |
base | xs:string
used by |
element | RmlsDpInformation/conditionCode
facets |
Kind | Value | Annotation
enumeration | I |
documentation
Normal, inactive state and should be removed (i.e. become invisible) from status displays on RMLS-NRN, see also TI 6140.31, RMLS Peabody User's Guide, and NAS-IC-51015108-01, Interface Control Document: Communications Remote Maintenance Monitoring (CRMM) Remote Monitoring Subsystem (RMS) Concentrator and Subdevices To Remote Monitoring Logging System (RMLS) National RMM Network (NRN) Interface.
enumeration | N |
documentation
Active, unacknowledged, alarm state (red status), see also TI 6140.31, RMLS Peabody User's Guide, and NAS-IC-51015108-01, Interface Control Document: Communications Remote Maintenance Monitoring (CRMM) Remote Monitoring Subsystem (RMS) Concentrator and Subdevices To Remote Monitoring Logging System (RMLS) National RMM Network (NRN) Interface.
enumeration | P |
documentation
Active, unacknowledged, alert/warning state (yellow status), see also TI 6140.31, RMLS Peabody User's Guide, and NAS-IC-51015108-01, Interface Control Document: Communications Remote Maintenance Monitoring (CRMM) Remote Monitoring Subsystem (RMS) Concentrator and Subdevices To Remote Monitoring Logging System (RMLS) National RMM Network (NRN) Interface.
enumeration | S |
documentation
Site Data Report (green status), see also TI 6140.31, RMLS Peabody User's Guide, and NAS-IC-51015108-01, Interface Control Document: Communications Remote Maintenance Monitoring (CRMM) Remote Monitoring Subsystem (RMS) Concentrator and Subdevices To Remote Monitoring Logging System (RMLS) National RMM Network (NRN) Interface.
enumeration | L |
documentation
Warning or alert state (yellow status), see also TI 6140.31, RMLS Peabody User's Guide, and NAS-IC-51015108-01, Interface Control Document: Communications Remote Maintenance Monitoring (CRMM) Remote Monitoring Subsystem (RMS) Concentrator and Subdevices To Remote Monitoring Logging System (RMLS) National RMM Network (NRN) Interface.
enumeration | A |
documentation
Alarm condition (red status), see also TI 6140.31, RMLS Peabody User's Guide, and NAS-IC-51015108-01, Interface Control Document: Communications Remote Maintenance Monitoring (CRMM) Remote Monitoring Subsystem (RMS) Concentrator and Subdevices To Remote Monitoring Logging System (RMLS) National RMM Network (NRN) Interface.
enumeration | C |
documentation
State change, see also TI 6140.31, RMLS Peabody User's Guide, and NAS-IC-51015108-01, Interface Control Document: Communications Remote Maintenance Monitoring (CRMM) Remote Monitoring Subsystem (RMS) Concentrator and Subdevices To Remote Monitoring Logging System (RMLS) National RMM Network (NRN) Interface.
enumeration | R |
documentation
Return to Normal (green status), see also TI 6140.31, RMLS Peabody User's Guide, and NAS-IC-51015108-01, Interface Control Document: Communications Remote Maintenance Monitoring (CRMM) Remote Monitoring Subsystem (RMS) Concentrator and Subdevices To Remote Monitoring Logging System (RMLS) National RMM Network (NRN) Interface.
annotation |
documentation
Status and condition information pertaining to an individual RMLS Data Point. (Reference: NAS-IC-51015108-01_RMLS_CMHP)
source | <xs:simpleType name="RmlsConditionCodeType"> <xs:annotation> <xs:documentation>Status and condition information pertaining to an individual RMLS Data Point. (Reference: NAS-IC-51015108-01_RMLS_CMHP)</xs:documentation> </xs:annotation> <xs:restriction base="xs:string"> <xs:enumeration value="I"> <xs:annotation> <xs:documentation>Normal, inactive state and should be removed (i.e. become invisible) from status displays on RMLS-NRN, see also TI 6140.31, RMLS Peabody User's Guide, and NAS-IC-51015108-01, Interface Control Document: Communications Remote Maintenance Monitoring (CRMM) Remote Monitoring Subsystem (RMS) Concentrator and Subdevices To Remote Monitoring Logging System (RMLS) National RMM Network (NRN) Interface.</xs:documentation> </xs:annotation> </xs:enumeration> <xs:enumeration value="N"> <xs:annotation> <xs:documentation>Active, unacknowledged, alarm state (red status), see also TI 6140.31, RMLS Peabody User's Guide, and NAS-IC-51015108-01, Interface Control Document: Communications Remote Maintenance Monitoring (CRMM) Remote Monitoring Subsystem (RMS) Concentrator and Subdevices To Remote Monitoring Logging System (RMLS) National RMM Network (NRN) Interface.</xs:documentation> </xs:annotation> </xs:enumeration> <xs:enumeration value="P"> <xs:annotation> <xs:documentation>Active, unacknowledged, alert/warning state (yellow status), see also TI 6140.31, RMLS Peabody User's Guide, and NAS-IC-51015108-01, Interface Control Document: Communications Remote Maintenance Monitoring (CRMM) Remote Monitoring Subsystem (RMS) Concentrator and Subdevices To Remote Monitoring Logging System (RMLS) National RMM Network (NRN) Interface.</xs:documentation> </xs:annotation> </xs:enumeration> <xs:enumeration value="S"> <xs:annotation> <xs:documentation>Site Data Report (green status), see also TI 6140.31, RMLS Peabody User's Guide, and NAS-IC-51015108-01, Interface Control Document: Communications Remote Maintenance Monitoring (CRMM) Remote Monitoring Subsystem (RMS) Concentrator and Subdevices To Remote Monitoring Logging System (RMLS) National RMM Network (NRN) Interface.</xs:documentation> </xs:annotation> </xs:enumeration> <xs:enumeration value="L"> <xs:annotation> <xs:documentation>Warning or alert state (yellow status), see also TI 6140.31, RMLS Peabody User's Guide, and NAS-IC-51015108-01, Interface Control Document: Communications Remote Maintenance Monitoring (CRMM) Remote Monitoring Subsystem (RMS) Concentrator and Subdevices To Remote Monitoring Logging System (RMLS) National RMM Network (NRN) Interface.</xs:documentation> </xs:annotation> </xs:enumeration> <xs:enumeration value="A"> <xs:annotation> <xs:documentation>Alarm condition (red status), see also TI 6140.31, RMLS Peabody User's Guide, and NAS-IC-51015108-01, Interface Control Document: Communications Remote Maintenance Monitoring (CRMM) Remote Monitoring Subsystem (RMS) Concentrator and Subdevices To Remote Monitoring Logging System (RMLS) National RMM Network (NRN) Interface.</xs:documentation> </xs:annotation> </xs:enumeration> <xs:enumeration value="C"> <xs:annotation> <xs:documentation>State change, see also TI 6140.31, RMLS Peabody User's Guide, and NAS-IC-51015108-01, Interface Control Document: Communications Remote Maintenance Monitoring (CRMM) Remote Monitoring Subsystem (RMS) Concentrator and Subdevices To Remote Monitoring Logging System (RMLS) National RMM Network (NRN) Interface.</xs:documentation> </xs:annotation> </xs:enumeration> <xs:enumeration value="R"> <xs:annotation> <xs:documentation>Return to Normal (green status), see also TI 6140.31, RMLS Peabody User's Guide, and NAS-IC-51015108-01, Interface Control Document: Communications Remote Maintenance Monitoring (CRMM) Remote Monitoring Subsystem (RMS) Concentrator and Subdevices To Remote Monitoring Logging System (RMLS) National RMM Network (NRN) Interface.</xs:documentation> </xs:annotation> </xs:enumeration> </xs:restriction> </xs:simpleType>

XML Schema documentation generated by XMLSpy Schema Editor http://www.altova.com/xmlspy