: Public <<XSDcomplexType>> Class

Created: | 3/22/2017 5:53:58 PM
Modified: | 3/16/2020 1:06:33 PM
Project: |
Author: | FAA
Version: | 4.0.0
Phase: |
Status: | Implemented
Complexity: | Easy
Difficulty: |
Priority: |
Multiplicity: |
Advanced: |
UUID: | {58CDB9CD-C361-4c95-A4D4-9825DD7114EB}
Appears In: | Qualifications, AssetIdentifier

Complex type containing the fsepFac, fsepFic, and fsepLocId.<br/>

- Attributes
- Associations From
- Tagged Values
- Advanced

Attribute
Public FsepFacType fsepFac
Details:
Alias: |
Initial: |
Stereotype: |
Ordered: |
Range: | Range:0 to 1
Transient: | False
Derived: | False
IsID: | False
pattern=[0-9A-Z]{2,5}
Notes: | The five- character alphanumeric field contains the type of entity in FSEP, including services. This is the field FAC_TYPE in the RMLS/FSEP database. Sample values include the following.<br/>ASR: Airport Surveillance Radar<br/>ATIS: Automatic Terminal Information System<br/>ATCT: Airport Traffic Control Tower<br/>BUECS: Backup Emergency Communications Service<br/>CFAD: Composite Flight Data Processing Service<br/>EADS: En Route Automation Display System<br/><br/>
Public FsepFicType fsepFic
Details:
Alias: |
Initial: |
Stereotype: |
Ordered: |
Range: | Range:0 to 1
Transient: | False
Derived: | False
IsID: | False
Notes: | The Facility Identification Code (FIC) provides the make, model, and class for identifying equipment in FSEP. The make and model codes make up the four-character FIC Code. The FIC Code is mandatory in all non-service records. The FIC Codes established prior to the release of older versions of Order 6000.5 are still valid and remain in the FSEP Desk guides until the equipment is retired from the NAS. Not all legacy codes are changed to the new FIC Code. This is the field FAC_CODE_FACILITY in the RMLS/FSEP database. Sample values include the following.<br/>ASR FICs: 53AC, 53AG, SC00<br/>GBAS FICs: NWA0<br/>TBFM FICs: 61UB, AE00<br/><br/>
Public FsepLocIdType fsepLocId
Details:
Alias: |
Initial: |
Stereotype: |
Ordered: |
Range: | Range:0 to 1
Transient: | False
Derived: | False
IsID: | False
Notes: | This three or four character field contains the city and state where the equipment is physically located. Location identifiers assignment process is detailed in Order 6000.5E, Chapter 3, Section 3.1 Location Identifier Process. This is the field FAC_IDENT in the RMLS/FSEP database but which is typically referred to as LOC_ID. There are three sources for a LOC_ID:<br/><ol> <li>A value from the IDENT column in the 7350.9.</li><li>A value from the IDENT column in the 7350.9 to which a single character suffix is added. The suffix is added when there is more than one instance of the same FSEP Facility at a specific location. An example is the Precision Approach Path Indicators (PAPI) at Boston Logan Airport. There are 4 of these, and each has a different LOC_ID derived from BOS, the identifier for Logan. These are BOS, BOSA, BOSB and BOSC.</li><li>A made up value starting with a Q. These are known as Q Identifiers and are created when there is no established identifier within 20 miles of the location of the FSEP Facility.</li></ol> Sample values include I90, DAL, TPA, CXYA, DCAP, PUB, ZDCC, DFWA.<br/>
Public integer fsepReferenceId
Details:
Alias: |
Initial: |
Stereotype: |
Ordered: |
Range: | Range:0 to 1
Transient: | False
Derived: | False
IsID: | False
Notes: | An internal asset record identifier used by FSEP.<br/>
Public FsepFacType previousFsepFac
Details:
Alias: |
Initial: |
Stereotype: |
Ordered: |
Range: | Range:0 to 1
Transient: | False
Derived: | False
IsID: | False
Notes: | The FsepFac previously associated with this asset, per Order 6000.5 Facility, Service, and Equipment Profile (FSEP).<br/>
Public FsepLocIdType previousFsepLocId
Details:
Alias: |
Initial: |
Stereotype: |
Ordered: |
Range: | Range:0 to 1
Transient: | False
Derived: | False
IsID: | False
Notes: | The FSEP Location Ident that was previously in use by the asset, per Order 6000.5 Facility, Service, and Equipment Profile (FSEP).<br/>

Element | Source Role | Target Role
«XSDcomplexType» AssetIdentifier Class | Name: | Name: fsepIdentifier FSEP asset identification information.
Details:
«XSDcomplexType» Qualification Class | Name: | Name: fsepIdentifier FSEP asset identification information.
Details:

Tag | Value
mixed | false
Details: Values: true | false Default: false Description: Determines whether this element may contain mixed element and character content. Refer to the W3C XML Schema recommendation
modelGroup | sequence
Details: Values: all | sequence | choice Default: sequence Description: Overrides the package-level default model group

Property | Value
isFinalSpecialization: | 0