: Public <<XSDcomplexType>> Class

Created: | 7/5/2016 7:46:14 AM
Modified: | 3/16/2020 1:14:15 PM
Project: |
Author: | FAA
Version: | 4.0.0
Phase: |
Status: | Implemented
Complexity: | Easy
Difficulty: |
Priority: |
Multiplicity: |
Advanced: |
UUID: | {140BE754-3792-4c13-898B-D1B91B2E3664}
Appears In: | Asset

Complex type containing the FSEP code, class code, and system code.<br/>

- Attributes
- Associations From
- Tagged Values
- Advanced

Attribute
Public DomainCodeType capabilityCode
Details:
Alias: |
Initial: |
Stereotype: |
Ordered: |
Range: | Range:0 to 1
Transient: | False
Derived: | False
IsID: | False
Notes: | As defined in FSEP Order 6000.5E, the first position of the FIC is a one position alpha code that classifies the entity by its primary capability. [Absence of a letter signifies an outdated code.] A: Automation, C: Communication, I: Infrastructure, M: Mission Support, N: Navigation/Landing, S: Surveillance, W: Weather.<br/>
Public CodeDescriptionType fsepClass
Details:
Alias: |
Initial: |
Stereotype: |
Ordered: |
Range: | Range:0 to 1
Transient: | False
Derived: | False
IsID: | False
Notes: | The container for the alphanumeric code further identifying equipment, as defined in the FSEP Desk Guide, and the associated description, per Order 6000.5 Facility, Service, and Equipment Profile (FSEP).<br/><br/>
Public FsepSystemCodeType fsepSystemCode
Details:
Alias: |
Initial: |
Stereotype: |
Ordered: |
Range: | Range:0 to 1
Transient: | False
Derived: | False
IsID: | False
Notes: | This code is a one-character numeric code that identifies the domain of the system within the NAS. This is also the first character numeric in the Facility Code/Class in the FSEP Data Dictionary (6000.5E, Appendix B). This is also the field FAC_CODE_SYSID in the RMLS/FSEP database. <br/>
Public String1Type powerCode
Details:
Alias: |
Initial: |
Stereotype: |
Ordered: |
Range: | Range:0 to 1
Transient: | False
Derived: | False
IsID: | False
Notes: | The power code indicates the chargeable power source for the primary asset, per Order 6000.5 Facility, Service, and Equipment Profile (FSEP).<br/>
Public CodeResponsibilityType responsibilityCode
Details:
Alias: |
Initial: |
Stereotype: |
Ordered: |
Range: | Range:0 to 1
Transient: | False
Derived: | False
IsID: | False
Notes: | The entity responsible for maintaining the asset.<br/>
Public CodeDescriptionType restorationPeriod
Details:
Alias: |
Initial: |
Stereotype: |
Ordered: |
Range: | Range:0 to 1
Transient: | False
Derived: | False
IsID: | False
Notes: | A code representing the allowable restoration response time for the asset, per Order 6000.5 Facility, Service, and Equipment Profile (FSEP).<br/>

Element | Source Role | Target Role
«XSDcomplexType» FsepOperationalInformation Class | Name: | Name: fsepCode FSEP code, class code, and system code.
Details:

Tag | Value
isCollection | false
Details: Values: true | false Default: false Description: Identifies the data type as an object collection.
mixed | false
Details: Values: true | false Default: false Description: Determines whether this element may contain mixed element and character content. Refer to the W3C XML Schema recommendation
modelGroup | sequence
Details: Values: all | sequence | choice Default: sequence Description: Overrides the package-level default model group
noPropertyType | false
Details: Values: false Default: false Description: Surpress creation of a standard property type that supports inline encoding (applies to ISO 19136:2007 encoding rule). Always set to false in INSPIRE.
xsdEncodingRule | iso19136_2007
Details: Values: iso19136_2007 | iso19139_2007 | iso19136_2007_INSPIRE_Extensions Default: iso19136_2007 Description: XML Schema encoding rule to apply

Property | Value
isFinalSpecialization: | 0