simpleType CodeInterruptConditionDescriptionType

namespace | https://mmixm.aero/base/4
type | restriction of xs:string
properties |
base | xs:string
used by |
element | InterruptReport/interruptType
facets |
Kind | Value | Annotation
enumeration | Full Interruption |
documentation
The interrupt condition is a full outage, see also TI 6140.33, Remote Monitoring and Logging System Operations Control Center (OCC) and Service Operation Center (SOC) Event Manager (EM) User's Guide.
enumeration | Informational Entry |
documentation
The log entry is for coordination purposes only, see also TI 6140.33, Remote Monitoring and Logging System Operations Control Center (OCC) and Service Operation Center (SOC) Event Manager (EM) User's Guide.
enumeration | Reduced Facility/Service Interruption |
documentation
The interruption or outage has resulted in a reduced service condition, see also TI 6140.33, Remote Monitoring and Logging System Operations Control Center (OCC) and Service Operation Center (SOC) Event Manager (EM) User's Guide.
enumeration | Reduced System/Equipment |
documentation
The interruption or outage has resulted in a reduced equipment condition, see also TI 6140.33, Remote Monitoring and Logging System Operations Control Center (OCC) and Service Operation Center (SOC) Event Manager (EM) User's Guide.
annotation |
documentation
TI 6140.33B OCC/SOC Event Manager User's Guide 5.1.2.2 Filter Events. Identifies the extent of the outage.
source | <xs:simpleType name="CodeInterruptConditionDescriptionType"> <xs:annotation> <xs:documentation>TI 6140.33B OCC/SOC Event Manager User's Guide 5.1.2.2 Filter Events. Identifies the extent of the outage.</xs:documentation> </xs:annotation> <xs:restriction base="xs:string"> <xs:enumeration value="Full Interruption"> <xs:annotation> <xs:documentation>The interrupt condition is a full outage, see also TI 6140.33, Remote Monitoring and Logging System Operations Control Center (OCC) and Service Operation Center (SOC) Event Manager (EM) User's Guide.</xs:documentation> </xs:annotation> </xs:enumeration> <xs:enumeration value="Informational Entry"> <xs:annotation> <xs:documentation>The log entry is for coordination purposes only, see also TI 6140.33, Remote Monitoring and Logging System Operations Control Center (OCC) and Service Operation Center (SOC) Event Manager (EM) User's Guide.</xs:documentation> </xs:annotation> </xs:enumeration> <xs:enumeration value="Reduced Facility/Service Interruption"> <xs:annotation> <xs:documentation>The interruption or outage has resulted in a reduced service condition, see also TI 6140.33, Remote Monitoring and Logging System Operations Control Center (OCC) and Service Operation Center (SOC) Event Manager (EM) User's Guide.</xs:documentation> </xs:annotation> </xs:enumeration> <xs:enumeration value="Reduced System/Equipment"> <xs:annotation> <xs:documentation>The interruption or outage has resulted in a reduced equipment condition, see also TI 6140.33, Remote Monitoring and Logging System Operations Control Center (OCC) and Service Operation Center (SOC) Event Manager (EM) User's Guide.</xs:documentation> </xs:annotation> </xs:enumeration> </xs:restriction> </xs:simpleType>

XML Schema documentation generated by XMLSpy Schema Editor http://www.altova.com/xmlspy