complexType RmlsDpInformation

diagram |
namespace | https://mmixm.aero/features/4
children | mx:conditionCode mx:criticality mx:description mx:dpId mx:rawValue mx:shortName
used by |
element | MonitoringEvent/rmlsDpInformation
annotation |
documentation
Complex type containing information specific to an RMLS Data Point.
source | <xs:complexType name="RmlsDpInformation"> <xs:annotation> <xs:documentation>Complex type containing information specific to an RMLS Data Point.</xs:documentation> </xs:annotation> <xs:sequence> <xs:element name="conditionCode" type="mx:RmlsConditionCodeType" minOccurs="0" maxOccurs="1"> <xs:annotation> <xs:documentation>Status and condition information pertaining to an individual RMLS Data Point.</xs:documentation> </xs:annotation> </xs:element> <xs:element name="criticality" type="mx:RmlsCriticalityCodeType" minOccurs="0" maxOccurs="1"> <xs:annotation> <xs:documentation>The criticality RMLS-NRN assigns to each RMLS Data Point reflecting the urgency of that component failing.</xs:documentation> </xs:annotation> </xs:element> <xs:element name="description" type="mb:String50Type" minOccurs="0" maxOccurs="1"> <xs:annotation> <xs:documentation>The description of the RMLS Data Point.</xs:documentation> </xs:annotation> </xs:element> <xs:element name="dpId" type="mb:RmlsHexId" minOccurs="0" maxOccurs="1"> <xs:annotation> <xs:documentation>The RMLS Data Point identifier, represented as a Hex Id.</xs:documentation> </xs:annotation> </xs:element> <xs:element name="rawValue" type="mb:String15Type" minOccurs="0" maxOccurs="1"> <xs:annotation> <xs:documentation>Unmediated status or measured value of a monitored RMLS Data Point.</xs:documentation> </xs:annotation> </xs:element> <xs:element name="shortName" type="mb:String10Type" minOccurs="0" maxOccurs="1"> <xs:annotation> <xs:documentation>The short name of the RMLS Data Point, limited to 10 characters.</xs:documentation> </xs:annotation> </xs:element> </xs:sequence> </xs:complexType>

element RmlsDpInformation/conditionCode

diagram |
namespace | https://mmixm.aero/features/4
type | mx:RmlsConditionCodeType
properties |
minOcc | 0
maxOcc | 1
content | simple
facets |
Kind | Value | Annotation
enumeration | I |
documentation
Normal, inactive state and should be removed (i.e. become invisible) from status displays on RMLS-NRN, see also TI 6140.31, RMLS Peabody User's Guide, and NAS-IC-51015108-01, Interface Control Document: Communications Remote Maintenance Monitoring (CRMM) Remote Monitoring Subsystem (RMS) Concentrator and Subdevices To Remote Monitoring Logging System (RMLS) National RMM Network (NRN) Interface.
enumeration | N |
documentation
Active, unacknowledged, alarm state (red status), see also TI 6140.31, RMLS Peabody User's Guide, and NAS-IC-51015108-01, Interface Control Document: Communications Remote Maintenance Monitoring (CRMM) Remote Monitoring Subsystem (RMS) Concentrator and Subdevices To Remote Monitoring Logging System (RMLS) National RMM Network (NRN) Interface.
enumeration | P |
documentation
Active, unacknowledged, alert/warning state (yellow status), see also TI 6140.31, RMLS Peabody User's Guide, and NAS-IC-51015108-01, Interface Control Document: Communications Remote Maintenance Monitoring (CRMM) Remote Monitoring Subsystem (RMS) Concentrator and Subdevices To Remote Monitoring Logging System (RMLS) National RMM Network (NRN) Interface.
enumeration | S |
documentation
Site Data Report (green status), see also TI 6140.31, RMLS Peabody User's Guide, and NAS-IC-51015108-01, Interface Control Document: Communications Remote Maintenance Monitoring (CRMM) Remote Monitoring Subsystem (RMS) Concentrator and Subdevices To Remote Monitoring Logging System (RMLS) National RMM Network (NRN) Interface.
enumeration | L |
documentation
Warning or alert state (yellow status), see also TI 6140.31, RMLS Peabody User's Guide, and NAS-IC-51015108-01, Interface Control Document: Communications Remote Maintenance Monitoring (CRMM) Remote Monitoring Subsystem (RMS) Concentrator and Subdevices To Remote Monitoring Logging System (RMLS) National RMM Network (NRN) Interface.
enumeration | A |
documentation
Alarm condition (red status), see also TI 6140.31, RMLS Peabody User's Guide, and NAS-IC-51015108-01, Interface Control Document: Communications Remote Maintenance Monitoring (CRMM) Remote Monitoring Subsystem (RMS) Concentrator and Subdevices To Remote Monitoring Logging System (RMLS) National RMM Network (NRN) Interface.
enumeration | C |
documentation
State change, see also TI 6140.31, RMLS Peabody User's Guide, and NAS-IC-51015108-01, Interface Control Document: Communications Remote Maintenance Monitoring (CRMM) Remote Monitoring Subsystem (RMS) Concentrator and Subdevices To Remote Monitoring Logging System (RMLS) National RMM Network (NRN) Interface.
enumeration | R |
documentation
Return to Normal (green status), see also TI 6140.31, RMLS Peabody User's Guide, and NAS-IC-51015108-01, Interface Control Document: Communications Remote Maintenance Monitoring (CRMM) Remote Monitoring Subsystem (RMS) Concentrator and Subdevices To Remote Monitoring Logging System (RMLS) National RMM Network (NRN) Interface.
annotation |
documentation
Status and condition information pertaining to an individual RMLS Data Point.
source | <xs:element name="conditionCode" type="mx:RmlsConditionCodeType" minOccurs="0" maxOccurs="1"> <xs:annotation> <xs:documentation>Status and condition information pertaining to an individual RMLS Data Point.</xs:documentation> </xs:annotation> </xs:element>

element RmlsDpInformation/criticality

diagram |
namespace | https://mmixm.aero/features/4
type | mx:RmlsCriticalityCodeType
properties |
minOcc | 0
maxOcc | 1
content | simple
facets |
Kind | Value | Annotation
enumeration | 1 |
documentation
Indicates the system is out of service (OTS) or possible service impacting alarm/alert. Definition based on Appendix K, NAS Event Management and Coordination (NEMAC) SOP.
enumeration | 2 |
documentation
Imminent failure or service impacting Loss of Redundancy (LOR). Definition based on Appendix K, NAS Event Management and Coordination (NEMAC) SOP.
enumeration | 3 |
documentation
Imminent failure or service impacting Loss of Redundancy (LOR). Definition based on Appendix K, NAS Event Management and Coordination (NEMAC) SOP.
enumeration | 4 |
documentation
A RMLS Data Point approaching an out of tolerance threshold or an element failure not causing a service impacting LOR or OTS condition. Definition based on Appendix K, NAS Event Management and Coordination (NEMAC) SOP.
enumeration | 5 |
documentation
A RMLS Data Point approaching an out of tolerance threshold or an element failure not causing a service impacting LOR or OTS condition. Definition based on Appendix K, NAS Event Management and Coordination (NEMAC) SOP.
enumeration | 6 |
documentation
A RMLS Data Point approaching an out of tolerance threshold or an element failure not causing a service impacting LOR or OTS condition. Definition based on Appendix K, NAS Event Management and Coordination (NEMAC) SOP.
enumeration | 7 |
documentation
A RMLS Data Point approaching an out of tolerance threshold or an element failure not causing a service impacting LOR or OTS condition. Definition based on Appendix K, NAS Event Management and Coordination (NEMAC) SOP.
enumeration | 8 |
documentation
A RMLS Data Point approaching an out of tolerance threshold or an element failure not causing a service impacting LOR or OTS condition. Definition based on Appendix K, NAS Event Management and Coordination (NEMAC) SOP.
enumeration | 9 |
documentation
A RMLS Data Point approaching an out of tolerance threshold or an element failure not causing a service impacting LOR or OTS condition. Definition based on Appendix K, NAS Event Management and Coordination (NEMAC) SOP.
annotation |
documentation
The criticality RMLS-NRN assigns to each RMLS Data Point reflecting the urgency of that component failing.
source | <xs:element name="criticality" type="mx:RmlsCriticalityCodeType" minOccurs="0" maxOccurs="1"> <xs:annotation> <xs:documentation>The criticality RMLS-NRN assigns to each RMLS Data Point reflecting the urgency of that component failing.</xs:documentation> </xs:annotation> </xs:element>

element RmlsDpInformation/description

diagram |
namespace | https://mmixm.aero/features/4
type | mb:String50Type
properties |
minOcc | 0
maxOcc | 1
content | simple
facets |
Kind | Value | Annotation
maxLength | 50 |
annotation |
documentation
The description of the RMLS Data Point.
source | <xs:element name="description" type="mb:String50Type" minOccurs="0" maxOccurs="1"> <xs:annotation> <xs:documentation>The description of the RMLS Data Point.</xs:documentation> </xs:annotation> </xs:element>

element RmlsDpInformation/dpId

diagram |
namespace | https://mmixm.aero/features/4
type | mb:RmlsHexId
properties |
minOcc | 0
maxOcc | 1
content | simple
facets |
Kind | Value | Annotation
pattern | [0-9A-F]{0,2}x?[0-9A-F]{1,2} |
annotation |
documentation
The RMLS Data Point identifier, represented as a Hex Id.
source | <xs:element name="dpId" type="mb:RmlsHexId" minOccurs="0" maxOccurs="1"> <xs:annotation> <xs:documentation>The RMLS Data Point identifier, represented as a Hex Id.</xs:documentation> </xs:annotation> </xs:element>

element RmlsDpInformation/rawValue

diagram |
namespace | https://mmixm.aero/features/4
type | mb:String15Type
properties |
minOcc | 0
maxOcc | 1
content | simple
facets |
Kind | Value | Annotation
maxLength | 15 |
annotation |
documentation
Unmediated status or measured value of a monitored RMLS Data Point.
source | <xs:element name="rawValue" type="mb:String15Type" minOccurs="0" maxOccurs="1"> <xs:annotation> <xs:documentation>Unmediated status or measured value of a monitored RMLS Data Point.</xs:documentation> </xs:annotation> </xs:element>

element RmlsDpInformation/shortName

diagram |
namespace | https://mmixm.aero/features/4
type | mb:String10Type
properties |
minOcc | 0
maxOcc | 1
content | simple
facets |
Kind | Value | Annotation
maxLength | 10 |
annotation |
documentation
The short name of the RMLS Data Point, limited to 10 characters.
source | <xs:element name="shortName" type="mb:String10Type" minOccurs="0" maxOccurs="1"> <xs:annotation> <xs:documentation>The short name of the RMLS Data Point, limited to 10 characters.</xs:documentation> </xs:annotation> </xs:element>

XML Schema documentation generated by XMLSpy Schema Editor http://www.altova.com/xmlspy