: Public <<XSDcomplexType>> Class

Created: | 8/6/2024 4:22:24 PM
Modified: | 8/12/2024 11:52:14 AM
Project: |
Author: | FAA
Version: | 4.0.0
Phase: |
Status: | Implemented
Complexity: | Easy
Difficulty: |
Priority: |
Multiplicity: |
Advanced: |
UUID: | {F8A18814-ABE6-43e8-83BC-E31D99CF4C94}
Appears In: | Asset

Location information associated with the asset, such as location identifiers for associated remote command and control site or service delivery point.<br/>

- Attributes
- Associations From
- Tagged Values
- Advanced

Attribute
Public Location airTrafficLocation
Details:
Alias: |
Initial: |
Stereotype: |
Ordered: |
Range: | Range:0 to 1
Transient: | False
Derived: | False
IsID: | False
Notes: | Location responsible for the Air Traffic associated with the asset.<br/>
Public Location buildingLocation
Details:
Alias: |
Initial: |
Stereotype: |
Ordered: |
Range: | Range:0 to 1
Transient: | False
Derived: | False
IsID: | False
Notes: | Identifies the building where the assets are located or are supporting, per FAA 6000.5 Facility, Service, and Equipment Profile (FSEP), Appendix B: Facility/Service Data Definitions.<br/>
Public Location commandLocation
Details:
Alias: |
Initial: |
Stereotype: |
Ordered: |
Range: | Range:0 to 1
Transient: | False
Derived: | False
IsID: | False
Notes: | Location that hosts the hardware which is responsible for sending remote commands to the asset.<br/>
Public Location controlLocation
Details:
Alias: |
Initial: |
Stereotype: |
Ordered: |
Range: | Range:0 to 1
Transient: | False
Derived: | False
IsID: | False
Notes: | This location exercises control over the asset, such as initiating a remote reset, per FSEP Desk Guide.<br/>
Public Location monitorLocation
Details:
Alias: |
Initial: |
Stereotype: |
Ordered: |
Range: | Range:0 to 1
Transient: | False
Derived: | False
IsID: | False
Notes: | Location that is responsible for reporting, coordinating, and/or monitoring the asset, such as the Security Operations Center (SOC), Control Centers, or Headquarters-based organizations, per FAA 6000.5 Facility, Service, and Equipment Profile (FSEP), Appendix B: Facility/Service Data Definitions.<br/>
Public CodeRegionType previousRegionCode
Details:
Alias: |
Initial: |
Stereotype: |
Ordered: |
Range: | Range:0 to 1
Transient: | False
Derived: | False
IsID: | False
Notes: | The last NAS region associated with the operational asset, prior to the current region, if the region has changed.<br/>
Public Location primaryLocation
Details:
Alias: |
Initial: |
Stereotype: |
Ordered: |
Range: | Range:0 to 1
Transient: | False
Derived: | False
IsID: | False
Notes: | Location of the primary maintenance office associated with the asset, per FAA 6000.5 Facility, Service, and Equipment Profile (FSEP), Appendix B: Facility/Service Data Definitions. Supplementary information may include travel time to the asset and number of trips.<br/>
Public CodeRegionType regionCode
Details:
Alias: |
Initial: |
Stereotype: |
Ordered: |
Range: | Range:0 to 1
Transient: | False
Derived: | False
IsID: | False
Notes: | The code for the NAS region associated with the operational asset.<br/>
Public Location remoteLocation
Details:
Alias: |
Initial: |
Stereotype: |
Ordered: |
Range: | Range:0 to 1
Transient: | False
Derived: | False
IsID: | False
Notes: | The remote location associated with the asset, per the FSEP Desk Guide.<br/>
Public Location serviceDeliveryPointLocation
Details:
Alias: |
Initial: |
Stereotype: |
Ordered: |
Range: | Range:0 to 1
Transient: | False
Derived: | False
IsID: | False
Notes: | Location to which Air Traffic Services are delivered, per FAA 6000.5 Facility, Service, and Equipment Profile (FSEP), Appendix B: Facility/Service Data Definitions.<br/>

Element | Source Role | Target Role
«XSDcomplexType» FsepOperationalInformation Class | Name: | Name: associatedLocations Location information associated with the asset, such as location identifiers for associated remote command and control site or service delivery point.
Details:

Tag | Value
mixed | false
Details: Values: true | false Default: false Description: Determines whether this element may contain mixed element and character content. Refer to the W3C XML Schema recommendation
modelGroup | sequence
Details: Values: all | sequence | choice Default: sequence Description: Overrides the package-level default model group

Property | Value
isFinalSpecialization: | 0