complexType LoggingEvent

diagram |
namespace | https://mmixm.aero/features/4
children | mx:additionalInformation mx:alarm mx:arrivalDeparture mx:assignmentInformation mx:comment mx:createdBy mx:createdDateTime mx:creatorLocation mx:equipmentModification mx:fsepOperationalInformationSnapshot mx:interruptReport mx:logCoordination mx:loggingCode mx:logId mx:maintenanceActivity mx:modifiedBy mx:modifiedDateTime mx:notamInformation mx:periodicMaintenance mx:reportLevel mx:status mx:summary
used by |
element | Asset/loggingEvent
annotation |
documentation
Complex type containing logging event information.
source | <xs:complexType name="LoggingEvent"> <xs:annotation> <xs:documentation>Complex type containing logging event information.</xs:documentation> </xs:annotation> <xs:sequence> <xs:element name="additionalInformation" type="mb:AdditionalInformation" minOccurs="0" maxOccurs="1"> <xs:annotation> <xs:documentation>Additional information about a Logging event.</xs:documentation> </xs:annotation> </xs:element> <xs:element name="alarm" type="mx:Alarm" minOccurs="0" maxOccurs="1"> <xs:annotation> <xs:documentation>Alarm information associated with a logging event.</xs:documentation> </xs:annotation> </xs:element> <xs:element name="arrivalDeparture" type="mx:ArrivalDeparture" minOccurs="0" maxOccurs="1"> <xs:annotation> <xs:documentation>Technicians' travel information, such as arrival and departure times, and travel duration.</xs:documentation> </xs:annotation> </xs:element> <xs:element name="assignmentInformation" type="mx:AssignmentInformation" minOccurs="0" maxOccurs="1"> <xs:annotation> <xs:documentation>Information about assigned group and specialist.</xs:documentation> </xs:annotation> </xs:element> <xs:element name="comment" type="mb:String4000Type" minOccurs="0" maxOccurs="1"> <xs:annotation> <xs:documentation>Free text comment on the logging event, and can include detailed information, per JO 6040.15 National Airspace Performance Reporting Services (NAPRS).</xs:documentation> </xs:annotation> </xs:element> <xs:element name="createdBy" type="mb:ContactInformation" minOccurs="0" maxOccurs="1"> <xs:annotation> <xs:documentation>The contact information of the person who created the log entry.</xs:documentation> </xs:annotation> </xs:element> <xs:element name="createdDateTime" type="xs:dateTime" minOccurs="0" maxOccurs="1"> <xs:annotation> <xs:documentation>The time and date of when the log data was created.</xs:documentation> </xs:annotation> </xs:element> <xs:element name="creatorLocation" type="mb:Location" minOccurs="0" maxOccurs="1"> <xs:annotation> <xs:documentation>The organization/location of where the log data was created.</xs:documentation> </xs:annotation> </xs:element> <xs:element name="equipmentModification" type="mx:EquipmentModification" minOccurs="0" maxOccurs="1"> <xs:annotation> <xs:documentation>Information about an equipment modification event.</xs:documentation> </xs:annotation> </xs:element> <xs:element name="fsepOperationalInformationSnapshot" type="mx:FsepOperationalInformation" minOccurs="0" maxOccurs="1"> <xs:annotation> <xs:documentation>A static capture of the FSEP operational information associated with an asset, current at the time the event was logged.</xs:documentation> </xs:annotation> </xs:element> <xs:element name="interruptReport" type="mx:InterruptReport" minOccurs="0" maxOccurs="1"> <xs:annotation> <xs:documentation>Information about a break in continuity, the loss or unavailability of an asset, regardless of duration or cause.</xs:documentation> </xs:annotation> </xs:element> <xs:element name="logCoordination" type="mx:LogCoordination" minOccurs="0" maxOccurs="1"> <xs:annotation> <xs:documentation>Log coordination information, such as whether coordination is required, the status of coordination, and whether the coordination was performed.</xs:documentation> </xs:annotation> </xs:element> <xs:element name="loggingCode" type="mx:LoggingCode" minOccurs="0" maxOccurs="1"> <xs:annotation> <xs:documentation>Code information for a logging event, including the code category, the maintenance action code, and the supplemental code.</xs:documentation> </xs:annotation> </xs:element> <xs:element name="logId" type="mb:Integer22Type" minOccurs="0" maxOccurs="1"> <xs:annotation> <xs:documentation>This field contains the ID number of the log entry.</xs:documentation> </xs:annotation> </xs:element> <xs:element name="maintenanceActivity" type="mx:MaintenanceActivity" minOccurs="0" maxOccurs="1"> <xs:annotation> <xs:documentation>Maintenance activity information, including start and end time of the maintenance activity.</xs:documentation> </xs:annotation> </xs:element> <xs:element name="modifiedBy" type="mb:ContactInformation" minOccurs="0" maxOccurs="1"> <xs:annotation> <xs:documentation>The contact information of the person that modified the log data.</xs:documentation> </xs:annotation> </xs:element> <xs:element name="modifiedDateTime" type="xs:dateTime" minOccurs="0" maxOccurs="1"> <xs:annotation> <xs:documentation>The time and date of when the log entry was modified / updated. (e.g. YYYY-MM-DDTHH:MM:SS)</xs:documentation> </xs:annotation> </xs:element> <xs:element name="notamInformation" type="mx:NotamInformation" minOccurs="0" maxOccurs="1"> <xs:annotation> <xs:documentation>Information about associated NOTAMs.</xs:documentation> </xs:annotation> </xs:element> <xs:element name="periodicMaintenance" type="mx:PeriodicMaintenance" minOccurs="0" maxOccurs="1"> <xs:annotation> <xs:documentation>Information about a periodic maintenance logging event.</xs:documentation> </xs:annotation> </xs:element> <xs:element name="reportLevel" type="mb:String1Type" minOccurs="0" maxOccurs="1"> <xs:annotation> <xs:documentation>The report level of the log entry as defined in TI 6140.31 RMLS Peabody User's Guide. "N" indicates reportable per Order 6040.15 (NAPRS), "L" indicates reportable by local policy.</xs:documentation> </xs:annotation> </xs:element> <xs:element name="status" type="mb:CodeLogStatusDescriptionType" minOccurs="0" maxOccurs="1"> <xs:annotation> <xs:documentation>The status of the log entry, per TI 6140.33 OCC/SOC Event Manager User's Guide. (e.g. Closed/ open / void)</xs:documentation> </xs:annotation> </xs:element> <xs:element name="summary" type="mb:String255Type" minOccurs="0" maxOccurs="1"> <xs:annotation> <xs:documentation>A free-text summary of the logged event or activity conducted.</xs:documentation> </xs:annotation> </xs:element> </xs:sequence> </xs:complexType>

element LoggingEvent/additionalInformation

diagram |
namespace | https://mmixm.aero/features/4
type | mb:AdditionalInformation
properties |
minOcc | 0
maxOcc | 1
content | complex
children | mb:nameValue
annotation |
documentation
Additional information about a Logging event.
source | <xs:element name="additionalInformation" type="mb:AdditionalInformation" minOccurs="0" maxOccurs="1"> <xs:annotation> <xs:documentation>Additional information about a Logging event.</xs:documentation> </xs:annotation> </xs:element>

element LoggingEvent/alarm

diagram |
namespace | https://mmixm.aero/features/4
type | mx:Alarm
properties |
minOcc | 0
maxOcc | 1
content | complex
children | mx:information mx:inputParameter mx:remoteAction mx:remoteResponse
annotation |
documentation
Alarm information associated with a logging event.
source | <xs:element name="alarm" type="mx:Alarm" minOccurs="0" maxOccurs="1"> <xs:annotation> <xs:documentation>Alarm information associated with a logging event.</xs:documentation> </xs:annotation> </xs:element>

element LoggingEvent/arrivalDeparture

diagram |
namespace | https://mmixm.aero/features/4
type | mx:ArrivalDeparture
properties |
minOcc | 0
maxOcc | 1
content | complex
children | mx:actualTravelDuration mx:arrivalDateTime mx:departureDateTime
annotation |
documentation
Technicians' travel information, such as arrival and departure times, and travel duration.
source | <xs:element name="arrivalDeparture" type="mx:ArrivalDeparture" minOccurs="0" maxOccurs="1"> <xs:annotation> <xs:documentation>Technicians' travel information, such as arrival and departure times, and travel duration.</xs:documentation> </xs:annotation> </xs:element>

element LoggingEvent/assignmentInformation

diagram |
namespace | https://mmixm.aero/features/4
type | mx:AssignmentInformation
properties |
minOcc | 0
maxOcc | 1
content | complex
children | mx:assignedGroup mx:assignedSpecialist
annotation |
documentation
Information about assigned group and specialist.
source | <xs:element name="assignmentInformation" type="mx:AssignmentInformation" minOccurs="0" maxOccurs="1"> <xs:annotation> <xs:documentation>Information about assigned group and specialist.</xs:documentation> </xs:annotation> </xs:element>

element LoggingEvent/comment

diagram |
namespace | https://mmixm.aero/features/4
type | mb:String4000Type
properties |
minOcc | 0
maxOcc | 1
content | simple
facets |
Kind | Value | Annotation
maxLength | 4000 |
annotation |
documentation
Free text comment on the logging event, and can include detailed information, per JO 6040.15 National Airspace Performance Reporting Services (NAPRS).
source | <xs:element name="comment" type="mb:String4000Type" minOccurs="0" maxOccurs="1"> <xs:annotation> <xs:documentation>Free text comment on the logging event, and can include detailed information, per JO 6040.15 National Airspace Performance Reporting Services (NAPRS).</xs:documentation> </xs:annotation> </xs:element>

element LoggingEvent/createdBy

diagram |
namespace | https://mmixm.aero/features/4
type | mb:ContactInformation
properties |
minOcc | 0
maxOcc | 1
content | complex
children | mb:email mb:postalAddress mb:telephoneContact
annotation |
documentation
The contact information of the person who created the log entry.
source | <xs:element name="createdBy" type="mb:ContactInformation" minOccurs="0" maxOccurs="1"> <xs:annotation> <xs:documentation>The contact information of the person who created the log entry.</xs:documentation> </xs:annotation> </xs:element>

element LoggingEvent/createdDateTime

diagram |
namespace | https://mmixm.aero/features/4
type | xs:dateTime
properties |
minOcc | 0
maxOcc | 1
content | simple
annotation |
documentation
The time and date of when the log data was created.
source | <xs:element name="createdDateTime" type="xs:dateTime" minOccurs="0" maxOccurs="1"> <xs:annotation> <xs:documentation>The time and date of when the log data was created.</xs:documentation> </xs:annotation> </xs:element>

element LoggingEvent/creatorLocation

diagram |
namespace | https://mmixm.aero/features/4
type | mb:Location
properties |
minOcc | 0
maxOcc | 1
content | complex
children | mb:electronicLocation mb:faaLocation mb:geographicLocation mb:gsaAddress mb:physicalAddress
annotation |
documentation
The organization/location of where the log data was created.
source | <xs:element name="creatorLocation" type="mb:Location" minOccurs="0" maxOccurs="1"> <xs:annotation> <xs:documentation>The organization/location of where the log data was created.</xs:documentation> </xs:annotation> </xs:element>

element LoggingEvent/equipmentModification

diagram |
namespace | https://mmixm.aero/features/4
type | mx:EquipmentModification
properties |
minOcc | 0
maxOcc | 1
content | complex
children | mx:assetOrder mx:changeNumber mx:directiveLevel mx:modification mx:modificationType mx:projectCode
annotation |
documentation
Information about an equipment modification event.
source | <xs:element name="equipmentModification" type="mx:EquipmentModification" minOccurs="0" maxOccurs="1"> <xs:annotation> <xs:documentation>Information about an equipment modification event.</xs:documentation> </xs:annotation> </xs:element>

element LoggingEvent/fsepOperationalInformationSnapshot

diagram |
namespace | https://mmixm.aero/features/4
type | mx:FsepOperationalInformation
properties |
minOcc | 0
maxOcc | 1
content | complex
children | mx:airportRunway mx:assetStatusHistory mx:associatedLocations mx:frequencyCount mx:fsepCode mx:numberOfUnits mx:phoneContact mx:recordProvenance mx:regionalInformation mx:revisionId mx:staffedHours mx:tier
annotation |
documentation
A static capture of the FSEP operational information associated with an asset, current at the time the event was logged.
source | <xs:element name="fsepOperationalInformationSnapshot" type="mx:FsepOperationalInformation" minOccurs="0" maxOccurs="1"> <xs:annotation> <xs:documentation>A static capture of the FSEP operational information associated with an asset, current at the time the event was logged.</xs:documentation> </xs:annotation> </xs:element>

element LoggingEvent/interruptReport

diagram |
namespace | https://mmixm.aero/features/4
type | mx:InterruptReport
properties |
minOcc | 0
maxOcc | 1
content | complex
children | mx:acknowledgedBy mx:acknowledgedDateTime mx:acknowledgedFlag mx:airTrafficImpact mx:backupStatus mx:cause mx:continuityOfService mx:deviceProvenance mx:estimatedRepairDuration mx:eventType mx:failureInformation mx:followUpDateTime mx:impactLevel mx:independentEditFlag mx:interruptType mx:operationalContingency mx:pagedBackFlag mx:pagedOutFlag mx:pagedUpdateFlag mx:primeRecovery mx:remoteSaveFlag mx:reviewedFlag mx:unscheduledFlag
annotation |
documentation
Information about a break in continuity, the loss or unavailability of an asset, regardless of duration or cause.
source | <xs:element name="interruptReport" type="mx:InterruptReport" minOccurs="0" maxOccurs="1"> <xs:annotation> <xs:documentation>Information about a break in continuity, the loss or unavailability of an asset, regardless of duration or cause.</xs:documentation> </xs:annotation> </xs:element>

element LoggingEvent/logCoordination

diagram |
namespace | https://mmixm.aero/features/4
type | mx:LogCoordination
properties |
minOcc | 0
maxOcc | 1
content | complex
children | mx:coordinationFlag mx:coordinationStage mx:electronicFlag
annotation |
documentation
Log coordination information, such as whether coordination is required, the status of coordination, and whether the coordination was performed.
source | <xs:element name="logCoordination" type="mx:LogCoordination" minOccurs="0" maxOccurs="1"> <xs:annotation> <xs:documentation>Log coordination information, such as whether coordination is required, the status of coordination, and whether the coordination was performed.</xs:documentation> </xs:annotation> </xs:element>

element LoggingEvent/loggingCode

diagram |
namespace | https://mmixm.aero/features/4
type | mx:LoggingCode
properties |
minOcc | 0
maxOcc | 1
content | complex
children | mx:category mx:maintenanceAction mx:supplemental
annotation |
documentation
Code information for a logging event, including the code category, the maintenance action code, and the supplemental code.
source | <xs:element name="loggingCode" type="mx:LoggingCode" minOccurs="0" maxOccurs="1"> <xs:annotation> <xs:documentation>Code information for a logging event, including the code category, the maintenance action code, and the supplemental code.</xs:documentation> </xs:annotation> </xs:element>

element LoggingEvent/logId

diagram |
namespace | https://mmixm.aero/features/4
type | mb:Integer22Type
properties |
minOcc | 0
maxOcc | 1
content | simple
facets |
Kind | Value | Annotation
maxInclusive | 9999999999999999999999 |
annotation |
documentation
This field contains the ID number of the log entry.
source | <xs:element name="logId" type="mb:Integer22Type" minOccurs="0" maxOccurs="1"> <xs:annotation> <xs:documentation>This field contains the ID number of the log entry.</xs:documentation> </xs:annotation> </xs:element>

element LoggingEvent/maintenanceActivity

diagram |
namespace | https://mmixm.aero/features/4
type | mx:MaintenanceActivity
properties |
minOcc | 0
maxOcc | 1
content | complex
children | mx:activityEndDateTime mx:activityStartDateTime
annotation |
documentation
Maintenance activity information, including start and end time of the maintenance activity.
source | <xs:element name="maintenanceActivity" type="mx:MaintenanceActivity" minOccurs="0" maxOccurs="1"> <xs:annotation> <xs:documentation>Maintenance activity information, including start and end time of the maintenance activity.</xs:documentation> </xs:annotation> </xs:element>

element LoggingEvent/modifiedBy

diagram |
namespace | https://mmixm.aero/features/4
type | mb:ContactInformation
properties |
minOcc | 0
maxOcc | 1
content | complex
children | mb:email mb:postalAddress mb:telephoneContact
annotation |
documentation
The contact information of the person that modified the log data.
source | <xs:element name="modifiedBy" type="mb:ContactInformation" minOccurs="0" maxOccurs="1"> <xs:annotation> <xs:documentation>The contact information of the person that modified the log data.</xs:documentation> </xs:annotation> </xs:element>

element LoggingEvent/modifiedDateTime

diagram |
namespace | https://mmixm.aero/features/4
type | xs:dateTime
properties |
minOcc | 0
maxOcc | 1
content | simple
annotation |
documentation
The time and date of when the log entry was modified / updated. (e.g. YYYY-MM-DDTHH:MM:SS)
source | <xs:element name="modifiedDateTime" type="xs:dateTime" minOccurs="0" maxOccurs="1"> <xs:annotation> <xs:documentation>The time and date of when the log entry was modified / updated. (e.g. YYYY-MM-DDTHH:MM:SS)</xs:documentation> </xs:annotation> </xs:element>

element LoggingEvent/notamInformation

diagram |
namespace | https://mmixm.aero/features/4
type | mx:NotamInformation
properties |
minOcc | 0
maxOcc | 1
content | complex
children | mx:transactionId
annotation |
documentation
Information about associated NOTAMs.
source | <xs:element name="notamInformation" type="mx:NotamInformation" minOccurs="0" maxOccurs="1"> <xs:annotation> <xs:documentation>Information about associated NOTAMs.</xs:documentation> </xs:annotation> </xs:element>

element LoggingEvent/periodicMaintenance

diagram |
namespace | https://mmixm.aero/features/4
type | mx:PeriodicMaintenance
properties |
minOcc | 0
maxOcc | 1
content | complex
children | mx:assetCertification mx:assignmentNumber mx:description mx:earliestDateTime mx:groupClosureCode mx:latestDateTime mx:publication mx:scheduleDateTime mx:schedulingCode mx:task mx:unitTag
annotation |
documentation
Information about a periodic maintenance logging event.
source | <xs:element name="periodicMaintenance" type="mx:PeriodicMaintenance" minOccurs="0" maxOccurs="1"> <xs:annotation> <xs:documentation>Information about a periodic maintenance logging event.</xs:documentation> </xs:annotation> </xs:element>

element LoggingEvent/reportLevel

diagram |
namespace | https://mmixm.aero/features/4
type | mb:String1Type
properties |
minOcc | 0
maxOcc | 1
content | simple
facets |
Kind | Value | Annotation
maxLength | 1 |
annotation |
documentation
The report level of the log entry as defined in TI 6140.31 RMLS Peabody User's Guide. "N" indicates reportable per Order 6040.15 (NAPRS), "L" indicates reportable by local policy.
source | <xs:element name="reportLevel" type="mb:String1Type" minOccurs="0" maxOccurs="1"> <xs:annotation> <xs:documentation>The report level of the log entry as defined in TI 6140.31 RMLS Peabody User's Guide. "N" indicates reportable per Order 6040.15 (NAPRS), "L" indicates reportable by local policy.</xs:documentation> </xs:annotation> </xs:element>

element LoggingEvent/status

diagram |
namespace | https://mmixm.aero/features/4
type | mb:CodeLogStatusDescriptionType
properties |
minOcc | 0
maxOcc | 1
content | simple
facets |
Kind | Value | Annotation
enumeration | Closed |
documentation
Log is closed, facility/service been restored, per TI 6140.32, RMLS National Operations Control Center (NOCC) Event Manager User's Guide.
enumeration | Open |
documentation
Log is open, facility/service remains out of service, per TI 6140.32, RMLS National Operations Control Center (NOCC) Event Manager User's Guide.
enumeration | Void |
documentation
Log has been voided, per TI 6030.6 Simplified Automated Logging (SAL) User's Manual.
annotation |
documentation
The status of the log entry, per TI 6140.33 OCC/SOC Event Manager User's Guide. (e.g. Closed/ open / void)
source | <xs:element name="status" type="mb:CodeLogStatusDescriptionType" minOccurs="0" maxOccurs="1"> <xs:annotation> <xs:documentation>The status of the log entry, per TI 6140.33 OCC/SOC Event Manager User's Guide. (e.g. Closed/ open / void)</xs:documentation> </xs:annotation> </xs:element>

element LoggingEvent/summary

diagram |
namespace | https://mmixm.aero/features/4
type | mb:String255Type
properties |
minOcc | 0
maxOcc | 1
content | simple
facets |
Kind | Value | Annotation
maxLength | 255 |
annotation |
documentation
A free-text summary of the logged event or activity conducted.
source | <xs:element name="summary" type="mb:String255Type" minOccurs="0" maxOccurs="1"> <xs:annotation> <xs:documentation>A free-text summary of the logged event or activity conducted.</xs:documentation> </xs:annotation> </xs:element>

XML Schema documentation generated by XMLSpy Schema Editor http://www.altova.com/xmlspy