complexType ManufacturerIdentifier

diagram |
namespace | https://mmixm.aero/features/4
children | mx:manufacturerName mx:manufacturerPartNumber mx:nationalStockNumber mx:revisionNumber mx:serialNumber
used by |
element | AssetIdentifier/manufacturerIdentifier
annotation |
documentation
Complex type containing asset identifiers assigned by manufacturers.
source | <xs:complexType name="ManufacturerIdentifier"> <xs:annotation> <xs:documentation>Complex type containing asset identifiers assigned by manufacturers.</xs:documentation> </xs:annotation> <xs:sequence> <xs:element name="manufacturerName" type="mb:String50Type" minOccurs="0" maxOccurs="1"> <xs:annotation> <xs:documentation>A producer of manufactured assets: parts, equipment, and/or systems.</xs:documentation> </xs:annotation> </xs:element> <xs:element name="manufacturerPartNumber" type="mb:String50Type" minOccurs="0" maxOccurs="1"> <xs:annotation> <xs:documentation>Unique identifier for a part manufactured by a specific manufacturer.</xs:documentation> </xs:annotation> </xs:element> <xs:element name="nationalStockNumber" type="mb:String50Type" minOccurs="0" maxOccurs="1"> <xs:annotation> <xs:documentation>The NSN is a 13-digit code recognized by the US government, NATO and other countries of the form: 6240-00-357-7976. The first four digits are the Federal Supply Class (FSC), used to group like items. The next two are the Country of Origin code, and the remaining are sequentially assigned.</xs:documentation> </xs:annotation> </xs:element> <xs:element name="revisionNumber" type="mb:String50Type" minOccurs="0" maxOccurs="1"> <xs:annotation> <xs:documentation>The revision number for this asset, such as the software revision level/number as noted in the modification document, per TI 6030.6 Simplified Automated Logging (SAL) User's Manual. (e.g. 1, 2, etc.)</xs:documentation> </xs:annotation> </xs:element> <xs:element name="serialNumber" type="mb:String50Type" minOccurs="0" maxOccurs="1"> <xs:annotation> <xs:documentation>Serial number assigned by the manufacturer.</xs:documentation> </xs:annotation> </xs:element> </xs:sequence> </xs:complexType>

element ManufacturerIdentifier/manufacturerName

diagram |
namespace | https://mmixm.aero/features/4
type | mb:String50Type
properties |
minOcc | 0
maxOcc | 1
content | simple
facets |
Kind | Value | Annotation
maxLength | 50 |
annotation |
documentation
A producer of manufactured assets: parts, equipment, and/or systems.
source | <xs:element name="manufacturerName" type="mb:String50Type" minOccurs="0" maxOccurs="1"> <xs:annotation> <xs:documentation>A producer of manufactured assets: parts, equipment, and/or systems.</xs:documentation> </xs:annotation> </xs:element>

element ManufacturerIdentifier/manufacturerPartNumber

diagram |
namespace | https://mmixm.aero/features/4
type | mb:String50Type
properties |
minOcc | 0
maxOcc | 1
content | simple
facets |
Kind | Value | Annotation
maxLength | 50 |
annotation |
documentation
Unique identifier for a part manufactured by a specific manufacturer.
source | <xs:element name="manufacturerPartNumber" type="mb:String50Type" minOccurs="0" maxOccurs="1"> <xs:annotation> <xs:documentation>Unique identifier for a part manufactured by a specific manufacturer.</xs:documentation> </xs:annotation> </xs:element>

element ManufacturerIdentifier/nationalStockNumber

diagram |
namespace | https://mmixm.aero/features/4
type | mb:String50Type
properties |
minOcc | 0
maxOcc | 1
content | simple
facets |
Kind | Value | Annotation
maxLength | 50 |
annotation |
documentation
The NSN is a 13-digit code recognized by the US government, NATO and other countries of the form: 6240-00-357-7976. The first four digits are the Federal Supply Class (FSC), used to group like items. The next two are the Country of Origin code, and the remaining are sequentially assigned.
source | <xs:element name="nationalStockNumber" type="mb:String50Type" minOccurs="0" maxOccurs="1"> <xs:annotation> <xs:documentation>The NSN is a 13-digit code recognized by the US government, NATO and other countries of the form: 6240-00-357-7976. The first four digits are the Federal Supply Class (FSC), used to group like items. The next two are the Country of Origin code, and the remaining are sequentially assigned.</xs:documentation> </xs:annotation> </xs:element>

element ManufacturerIdentifier/revisionNumber

diagram |
namespace | https://mmixm.aero/features/4
type | mb:String50Type
properties |
minOcc | 0
maxOcc | 1
content | simple
facets |
Kind | Value | Annotation
maxLength | 50 |
annotation |
documentation
The revision number for this asset, such as the software revision level/number as noted in the modification document, per TI 6030.6 Simplified Automated Logging (SAL) User's Manual. (e.g. 1, 2, etc.)
source | <xs:element name="revisionNumber" type="mb:String50Type" minOccurs="0" maxOccurs="1"> <xs:annotation> <xs:documentation>The revision number for this asset, such as the software revision level/number as noted in the modification document, per TI 6030.6 Simplified Automated Logging (SAL) User's Manual. (e.g. 1, 2, etc.)</xs:documentation> </xs:annotation> </xs:element>

element ManufacturerIdentifier/serialNumber

diagram |
namespace | https://mmixm.aero/features/4
type | mb:String50Type
properties |
minOcc | 0
maxOcc | 1
content | simple
facets |
Kind | Value | Annotation
maxLength | 50 |
annotation |
documentation
Serial number assigned by the manufacturer.
source | <xs:element name="serialNumber" type="mb:String50Type" minOccurs="0" maxOccurs="1"> <xs:annotation> <xs:documentation>Serial number assigned by the manufacturer.</xs:documentation> </xs:annotation> </xs:element>

XML Schema documentation generated by XMLSpy Schema Editor http://www.altova.com/xmlspy