: Public <<XSDsimpleType>> Class

Created: | 8/14/2019 11:36:57 AM
Modified: | 2/14/2023 5:50:34 PM
Project: |
Author: | FAA
Version: | 4.0.0
Phase: |
Status: | Implemented
Complexity: | Easy
Difficulty: |
Priority: |
Multiplicity: |
Advanced: |
UUID: | {2D527955-2437-4925-B395-F5FC46851B1D}
Appears In: |

The Facility Identification Code (FIC) provides the make, model, and class for identifying equipment in FSEP. The make and model codes make up the four-character FIC Code. The FIC Code is mandatory in all non-service records. The FIC Codes established prior to the release of older versions of Order 6000.5 are still valid and remain in the FSEP Desk guides until the equipment is retired from the NAS. Not all legacy codes are changed to the new FIC Code. This is the field FAC_CODE_FACILITY in the RMLS/FSEP database. Sample values include the following.<br/>ASR FICs: 53AC, 53AG, SC00<br/>GBAS FICs: NWA0<br/>TBFM FICs: 61UB, AE00<br/><br/>

- Tagged Values
- Constraints
- Advanced
- Other Links

Tag | Value
derivation | restriction
Details: Values: restriction | list Default: restriction Description: Defines derivation type
pattern | [0-9A-Z]{4,5}
Details: Description: As defined by XML Schema Datatypes specification

Constraint | Type | Status
No attributes or associations | Invariant | Implemented
Details: This UML class may not have any attributes or associations originating from it.<br/>
Parent must be simpleType | Invariant | Implemented
Details: If a superclass is specified, it must also be a SimpleType<br/>

Property | Value
isFinalSpecialization: | 0

Object | Type | Connection | Direction | Notes
string | Class | Generalization | To |