complexType Cause

diagram |
namespace | https://mmixm.aero/features/4
children | mx:group mx:rawText mx:subgroup
used by |
element | InterruptReport/cause
annotation |
documentation
Contains information pertaining to the cause of an interruption.
source | <xs:complexType name="Cause"> <xs:annotation> <xs:documentation>Contains information pertaining to the cause of an interruption.</xs:documentation> </xs:annotation> <xs:sequence> <xs:element name="group" type="mb:CodeDescriptionType" minOccurs="0" maxOccurs="1"> <xs:annotation> <xs:documentation>Contains a descriptions field that indicates the cause and need for interruption report. (e.g. LINE (REQ. FOR CC 61/81))</xs:documentation> </xs:annotation> </xs:element> <xs:element name="rawText" type="mb:String50Type" minOccurs="0" maxOccurs="1"> <xs:annotation> <xs:documentation>A free form field that provides the user with the ability to further define the cause and its details, and could contain abbreviations (e.g. CN).</xs:documentation> </xs:annotation> </xs:element> <xs:element name="subgroup" type="mb:CodeDescriptionType" minOccurs="0" maxOccurs="1"> <xs:annotation> <xs:documentation>Contains further defined descriptions of the cause of interruption report. (e.g. CIRCUIT NOISY)</xs:documentation> </xs:annotation> </xs:element> </xs:sequence> </xs:complexType>

element Cause/group

diagram |
namespace | https://mmixm.aero/features/4
type | mb:CodeDescriptionType
properties |
minOcc | 0
maxOcc | 1
content | complex
children | mb:code mb:description
annotation |
documentation
Contains a descriptions field that indicates the cause and need for interruption report. (e.g. LINE (REQ. FOR CC 61/81))
source | <xs:element name="group" type="mb:CodeDescriptionType" minOccurs="0" maxOccurs="1"> <xs:annotation> <xs:documentation>Contains a descriptions field that indicates the cause and need for interruption report. (e.g. LINE (REQ. FOR CC 61/81))</xs:documentation> </xs:annotation> </xs:element>

element Cause/rawText

diagram |
namespace | https://mmixm.aero/features/4
type | mb:String50Type
properties |
minOcc | 0
maxOcc | 1
content | simple
facets |
Kind | Value | Annotation
maxLength | 50 |
annotation |
documentation
A free form field that provides the user with the ability to further define the cause and its details, and could contain abbreviations (e.g. CN).
source | <xs:element name="rawText" type="mb:String50Type" minOccurs="0" maxOccurs="1"> <xs:annotation> <xs:documentation>A free form field that provides the user with the ability to further define the cause and its details, and could contain abbreviations (e.g. CN).</xs:documentation> </xs:annotation> </xs:element>

element Cause/subgroup

diagram |
namespace | https://mmixm.aero/features/4
type | mb:CodeDescriptionType
properties |
minOcc | 0
maxOcc | 1
content | complex
children | mb:code mb:description
annotation |
documentation
Contains further defined descriptions of the cause of interruption report. (e.g. CIRCUIT NOISY)
source | <xs:element name="subgroup" type="mb:CodeDescriptionType" minOccurs="0" maxOccurs="1"> <xs:annotation> <xs:documentation>Contains further defined descriptions of the cause of interruption report. (e.g. CIRCUIT NOISY)</xs:documentation> </xs:annotation> </xs:element>

XML Schema documentation generated by XMLSpy Schema Editor http://www.altova.com/xmlspy